# IPv6.Link[x].IPSec

Enables or disables IPSec
for IPv6
on the specified Ethernet interface.

#### Syntax

IPv6.Link[x].IPSec = mode

x = index of the link entry

#### Access

Read/Write

#### Type

String

#### Default

NO

#### Allowed values

YES | NO

#### Example

IPv6.Link[1].IPSec = YES

#### Details

For information about using IPsec with the CG board IPv6 stack, refer to cgsetkey - Configuring IPv6 security keys and policies and RFC 2401 Security Architecture for the Internet Protocol (IPSec). For information about using board keywords to configure IPv6 Ethernet interfaces, refer to Configuring IPv6 Ethernet connections.

#### See also

IPv6.Link[x].ICMPRateLimit, IPv6.Link[x].HopLimit