# Sample board keyword files

This topic presents sample board keyword files for running NaturalConference on the following boards:

- AG 2000/400

- CG 6060/C

- CG 6565/C

## AG 2000/400 sample board keyword file

The following sample board keyword file sets up an AG 2000/400 board running eight loopstart protocols for an analog interface in mu-law, capable of handling 40 to 80 conferencing ports in a single conferencing resource with three DSPs.

## agpi2cnf_400.cfg
#
# This model of AG configuration file has to be used with
# an AG2000/400 with 8 LoopStart interfaces configured in mu-Law.
# One DSP is used for IVR and three DSPs are loaded with NaturalConference
# to form one conferencing resource containing three DSPs.
#
##
Clocking.HBus.ClockSource = OSC
Clocking.HBus.ClockMode = STANDALONE
# Protocols definition
TCPFiles[0] = nocc.tcp # "no trunk control" protocol
TCPFiles[1] = lps0.tcp # Loopstart protocol
# Slac Files Definition
#NetworkInterface.Analog[0..7].ConfigFile = a2usasl6.slc
#NetworkInterface.Analog[0..7].ConfigFile = a2eurlsc.slc
#NetworkInterface.Analog[0..7].ConfigFile = a2jpnsl6.slc
# Default Modules activated
DSP.C5x.DSPFiles[0] = callp
DSP.C5x.DSPFiles[1] = dtmf
DSP.C5x.DSPFiles[2] = mf
DSP.C5x.DSPFiles[3] = ptf
DSP.C5x.DSPFiles[4] = signal
DSP.C5x.DSPFiles[5] = tone
DSP.C5x.DSPFiles[6] = voice
DSP.C5x.DSPFiles[7] = rvoice
#DSP.C5x.DSPFiles[8] = wave
#DSP.C5x.DSPFiles[9] = oki
DLMFiles[0] = gtp.leo
DLMFiles[1] = voice.leo
DLMFiles[2] = svc.leo
XLaw = MU-LAW
###########################################################################
# #
# one group of three DSPs is loaded with NaturalConference to #
# form one conferencing resource containing three DSPs. #
# #
###########################################################################
DSP.C5x[1].Image = agcnfm.c54
DSP.C5x[2..3].Image = agcnfs.c54
ConferencingStream.Enable = YES

## CG 6060/C sample board keyword files

The following sample board keyword file sets up an IVR configuration with one conferencing resource on a CG 6060/C board:

#
# c6060cnf_ivr_nonspan.cfg
# CG 6060 configuration file
#
# This file configures the board to run NaturalConference in standalone
# mode (non-spanning).
#
Clocking.HBus.ClockMode = STANDALONE
Clocking.HBus.ClockSource = OSC
DSPStream.VoiceIdleCode[0..15] = 0x7F
DSPStream.SignalIdleCode[0..15] = 0x00
#---------------------------
# NOTE: T1 configuration
#---------------------------
NetworkInterface.T1E1[0..15].Type = T1
NetworkInterface.T1E1[0..15].Impedance = DSX1
NetworkInterface.T1E1[0..15].LineCode = B8ZS
NetworkInterface.T1E1[0..15].FrameType = ESF
NetworkInterface.T1E1[0..15].SignalingType = RAW
DSP.C5x[0..47].Libs = cg6klibu
DSP.C5x[0..47].XLaw = MU_LAW
#---------------------------
# NOTE: E1 configuration
#---------------------------
#NetworkInterface.T1E1[0..15].Type = E1
#NetworkInterface.T1E1[0..15].Impedance = G703_120_OHM
#NetworkInterface.T1E1[0..15].LineCode = HDB3
#NetworkInterface.T1E1[0..15].FrameType = CEPT
#NetworkInterface.T1E1[0..15].SignalingType = RAW
#DSP.C5x[0..47].Libs = cg6kliba
#DSP.C5x[0..47].XLaw = A_LAW
#---------------------------
# Hardware Echo Cancellation
# NOTE: it is in by pass by default
# NOTE: uncomment the following two keyword lines to enable and set the XLaw
# accordingly
#---------------------------
# HardwareEcho.EchoChipEnabled = YES
# HardwareEcho.XLaw = A_LAW
# NumTxTimeSlots, NumRxTimeSlots may be 16 or 32
DSP.C5x[0].NumTxTimeSlots = 16
DSP.C5x[0].NumRxTimeSlots = 16
DSP.C5x[0].CmdQStart = 0xE800
DSP.C5x[0].DataInQStart = 0xF800
DSP.C5x[0].DspOutQStart = 0xFB00
# The following is required when #timeslots = 32 (but not for 16)
#DSP.C5x[0].CmdQSize = 0x110
DSP.C5x[0].Files = cg6conf.f41
SwitchConnectMode = AllConstantDelay
ConferencingStream.Enable = YES
#---------------------------
# Resource management
#---------------------------
Resource[0].Name = RSC1
Resource[0].Size = 120
Resource[0].TCPs = nocc
Resource[0].StartTimeSlot = 0
################################################################
# Before modifying this resource definition string refer to the CG 6060
# Installation and Developers Manual.
# NOTE: echo.ln20_apt25 - echo running on DSP has been removed
# from resource definitions. We recommend user to use
# the hardware echo chip for echo cancellation instead.
#################################################################
Resource[0].Definitions = ( dtmf.det_all & ptf.det_2f & tone.gen & \
callp.gnc & ptf.det_4f & \
( (rvoice.rec_mulaw & rvoice.play_mulaw) | \
(rvoice.rec_alaw & rvoice.play_alaw) | \
(rvoice.rec_lin & rvoice.play_lin) | \
(voice.rec_16 & (voice.play_16_100 | voice.play_16_150 | voice.play_16_200)) | \
(voice.rec_24 & (voice.play_24_100 | voice.play_24_150 | voice.play_24_200)) | \
(voice.rec_32 & (voice.play_32_100 | voice.play_32_150 | voice.play_32_200)) | \
(voice.rec_64 & (voice.play_64_100 | voice.play_64_150 | voice.play_64_200)) | \
(wave.rec_11_16b & wave.play_11_16b) | \
(wave.rec_11_8b & wave.play_11_8b) | \
(oki.rec_24 & (oki.play_24_100 | oki.play_24_150 | oki.play_24_200)) | \
(oki.rec_32 & (oki.play_32_100 | oki.play_32_150 | oki.play_32_200)) | \
(ima.rec_24 & ima.play_24) | \
(ima.rec_32 & ima.play_32) | \
(gsm_ms.frgsm_rec & gsm_ms.frgsm_play) | \
g726.rec_32 | g726.play_32) )
# NOTE: If the DSP cores listed below do not exist on the board, the DSP cores
# will be ignored and will not be booted or used.
Resource[0].Dsps = 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 \
24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 \
44 45 46 47
DebugMask = 0x0

The following sample board keyword file sets up an IVR configuration with one conferencing resource spanning two DSPs on a CG 6060/C board:

#
# c6060cnf_ivr_span.cfg
# CG6060 configuration file
#
# This file configures the board to run Natural Conferencing in spanning mode.
#
Clocking.HBus.ClockMode = STANDALONE
Clocking.HBus.ClockSource = OSC
DSPStream.VoiceIdleCode[0..15] = 0x7F
DSPStream.SignalIdleCode[0..15] = 0x00
#---------------------------
# NOTE: T1 configuration
#---------------------------
NetworkInterface.T1E1[0..15].Type = T1
NetworkInterface.T1E1[0..15].Impedance = DSX1
NetworkInterface.T1E1[0..15].LineCode = B8ZS
NetworkInterface.T1E1[0..15].FrameType = ESF
NetworkInterface.T1E1[0..15].SignalingType = RAW
DSP.C5x[0..47].Libs = cg6klibu
DSP.C5x[0..47].XLaw = MU_LAW
#---------------------------
# NOTE: E1 configuration
#---------------------------
#NetworkInterface.T1E1[0..15].Type = E1
#NetworkInterface.T1E1[0..15].Impedance = G703_120_OHM
#NetworkInterface.T1E1[0..15].LineCode = HDB3
#NetworkInterface.T1E1[0..15].FrameType = CEPT
#NetworkInterface.T1E1[0..15].SignalingType = RAW
#DSP.C5x[0..47].Libs = cg6kliba
#DSP.C5x[0..47].XLaw = A_LAW
#---------------------------
# Hardware Echo Cancellation
# NOTE: it is in by pass by default
# NOTE: uncomment the following two keyword lines to enable and set the XLaw accordingly
#---------------------------
# HardwareEcho.EchoChipEnabled = YES
# HardwareEcho.XLaw = A_LAW
# NumTxTimeSlots, NumRxTimeSlots may be 16 or 32
DSP.C5x[0..1].NumTxTimeSlots = 16
DSP.C5x[0..1].NumRxTimeSlots = 16
DSP.C5x[0..1].CmdQStart = 0xE800
DSP.C5x[0..1].DataInQStart = 0xF800
DSP.C5x[0..1].DspOutQStart = 0xFB00
# The following is required when #timeslots = 32 (but not for 16)
#DSP.C5x[0..1].CmdQSize = 0x110
DSP.C5x[0..1].Libs[1] = cg6mslib
DSP.C5x[0].Files = cgcnfm
DSP.C5x[1].Files = cgcnfs
SwitchConnectMode = AllConstantDelay
ConferencingStream.Enable = YES
#---------------------------
# Resource management
#---------------------------
Resource[0].Name = RSC1
Resource[0].Size = 120
Resource[0].TCPs = nocc
Resource[0].StartTimeSlot = 0
################################################################
# Before modifying this resource definition string refer to the CG 6060
# Installation and Developers Manual.
# NOTE: echo.ln20_apt25 - echo running on DSP has been removed
# from resource definitions. We recommend user to use
# the hardware echo chip for echo cancellation instead
#################################################################
Resource[0].Definitions = ( dtmf.det_all & ptf.det_2f & tone.gen & \
callp.gnc & ptf.det_4f & \
( (rvoice.rec_mulaw & rvoice.play_mulaw) | \
(rvoice.rec_alaw & rvoice.play_alaw) | \
(rvoice.rec_lin & rvoice.play_lin) | \
(voice.rec_16 & (voice.play_16_100 | voice.play_16_150 | voice.play_16_200)) | \
(voice.rec_24 & (voice.play_24_100 | voice.play_24_150 | voice.play_24_200)) | \
(voice.rec_32 & (voice.play_32_100 | voice.play_32_150 | voice.play_32_200)) | \
(voice.rec_64 & (voice.play_64_100 | voice.play_64_150 | voice.play_64_200)) | \
(wave.rec_11_16b & wave.play_11_16b) | \
(wave.rec_11_8b & wave.play_11_8b) | \
(oki.rec_24 & (oki.play_24_100 | oki.play_24_150 | oki.play_24_200)) | \
(oki.rec_32 & (oki.play_32_100 | oki.play_32_150 | oki.play_32_200)) | \
(ima.rec_24 & ima.play_24) | \
(ima.rec_32 & ima.play_32) | \
(gsm_ms.frgsm_rec & gsm_ms.frgsm_play) | \
g726.rec_32 | g726.play_32) )
# NOTE: If the DSP cores listed below do not exist on the board, the DSP cores will
# be ignored and will not be booted or used
Resource[0].Dsps = 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 \
24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 \
43 44 45 46 47
DebugMask = 0x0

## CG 6565/C sample board keyword files

The following sample board keyword file sets up an IVR configuration with one conferencing resource on a CG 6565/C board:

#
# c565cnf_ivr_nonspan.cfg
# CG 6565 configuration file
#
# This file configures the board to run NautralConference in standalone
# mode (non-spanning).
#
Clocking.HBus.ClockMode = STANDALONE
Clocking.HBus.ClockSource = OSC
DSPStream.VoiceIdleCode[0..15] = 0x7F
DSPStream.SignalIdleCode[0..15] = 0x00
#---------------------------
# NOTE: T1 configuration
#---------------------------
NetworkInterface.T1E1[0..15].Type = T1
NetworkInterface.T1E1[0..15].Impedance = DSX1
NetworkInterface.T1E1[0..15].LineCode = B8ZS
NetworkInterface.T1E1[0..15].FrameType = ESF
NetworkInterface.T1E1[0..15].SignalingType = RAW
DSP.C5x[0..95].Libs = cg6klibu
DSP.C5x[0..95].XLaw = MU_LAW
#---------------------------
# NOTE: E1 configuration
#---------------------------
#NetworkInterface.T1E1[0..15].Type = E1
#NetworkInterface.T1E1[0..15].Impedance = G703_120_OHM
#NetworkInterface.T1E1[0..15].LineCode = HDB3
#NetworkInterface.T1E1[0..15].FrameType = CEPT
#NetworkInterface.T1E1[0..15].SignalingType = RAW
#DSP.C5x[0..95].Libs = cg6kliba
#DSP.C5x[0..95].XLaw = A_LAW
#---------------------------
# Hardware Echo Cancellation
# NOTE: it is in by pass by default
# NOTE: uncomment the following two keyword lines to enable and set the XLaw
# accordingly
#---------------------------
# HardwareEcho.EchoChipEnabled = YES
# HardwareEcho.XLaw = A_LAW
# NumTxTimeSlots, NumRxTimeSlots may be 16 or 32
DSP.C5x[0].NumTxTimeSlots = 16
DSP.C5x[0].NumRxTimeSlots = 16
DSP.C5x[0].CmdQStart = 0xE800
DSP.C5x[0].DataInQStart = 0xF800
DSP.C5x[0].DspOutQStart = 0xFB00
# The following is required when #timeslots = 32 (but not for 16)
#DSP.C5x[0].CmdQSize = 0x110
DSP.C5x[0].Files = cg6conf.f41
SwitchConnectMode = AllConstantDelay
ConferencingStream.Enable = YES
#---------------------------
# Resource management
#---------------------------
Resource[0].Name = RSC1
Resource[0].Size = 120
Resource[0].TCPs = nocc
Resource[0].StartTimeSlot = 0
################################################################
# Before modifying this resource definition string refer to the CG 6565
# Installation and Developers Manual.
# NOTE: echo.ln20_apt25 - echo running on DSP has been removed
# from resource definitions. We recommend user to use
# the hardware echo chip for echo cancellation instead.
#################################################################
Resource[0].Definitions = ( dtmf.det_all & ptf.det_2f & tone.gen & \
callp.gnc & ptf.det_4f & \
( (rvoice.rec_mulaw & rvoice.play_mulaw) | \
(rvoice.rec_alaw & rvoice.play_alaw) | \
(rvoice.rec_lin & rvoice.play_lin) | \
(voice.rec_16 & (voice.play_16_100 | voice.play_16_150 | voice.play_16_200)) | \
(voice.rec_24 & (voice.play_24_100 | voice.play_24_150 | voice.play_24_200)) | \
(voice.rec_32 & (voice.play_32_100 | voice.play_32_150 | voice.play_32_200)) | \
(voice.rec_64 & (voice.play_64_100 | voice.play_64_150 | voice.play_64_200)) | \
(wave.rec_11_16b & wave.play_11_16b) | \
(wave.rec_11_8b & wave.play_11_8b) | \
(oki.rec_24 & (oki.play_24_100 | oki.play_24_150 | oki.play_24_200)) | \
(oki.rec_32 & (oki.play_32_100 | oki.play_32_150 | oki.play_32_200)) | \
(ima.rec_24 & ima.play_24) | \
(ima.rec_32 & ima.play_32) | \
(gsm_ms.frgsm_rec & gsm_ms.frgsm_play) | \
g726.rec_32 | g726.play_32) )
# NOTE: If the DSP cores listed below do not exist on the board, the DSP cores
# will be ignored and will not be booted or used
Resource[0].Dsps = 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 \
24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 \
44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 \
64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 \
84 85 86 87 88 89 90 91 92 93 94 95
DebugMask = 0x0

The following sample board keyword file sets up an IVR configuration with one conferencing resource spanning two DSPs on a CG 6565/C board:

#
# c565cnf_ivr_span.cfg
# CG 6565 configuration file
#
# This file configures the board to run Natural Conferencing in spanning mode.
#
Clocking.HBus.ClockMode = STANDALONE
Clocking.HBus.ClockSource = OSC
DSPStream.VoiceIdleCode[0..15] = 0x7F
DSPStream.SignalIdleCode[0..15] = 0x00
#---------------------------
# NOTE: T1 configuration
#---------------------------
NetworkInterface.T1E1[0..15].Type = T1
NetworkInterface.T1E1[0..15].Impedance = DSX1
NetworkInterface.T1E1[0..15].LineCode = B8ZS
NetworkInterface.T1E1[0..15].FrameType = ESF
NetworkInterface.T1E1[0..15].SignalingType = RAW
DSP.C5x[0..95].Libs = cg6klibu
DSP.C5x[0..95].XLaw = MU_LAW
#---------------------------
# NOTE: E1 configuration
#---------------------------
#NetworkInterface.T1E1[0..15].Type = E1
#NetworkInterface.T1E1[0..15].Impedance = G703_120_OHM
#NetworkInterface.T1E1[0..15].LineCode = HDB3
#NetworkInterface.T1E1[0..15].FrameType = CEPT
#NetworkInterface.T1E1[0..15].SignalingType = RAW
#DSP.C5x[0..95].Libs = cg6kliba
#DSP.C5x[0..95].XLaw = A_LAW
#---------------------------
# Hardware Echo Cancellation
# NOTE: it is in by pass by default
# NOTE: uncomment the following two keyword lines to enable and set the XLaw accordingly
#---------------------------
# HardwareEcho.EchoChipEnabled = YES
# HardwareEcho.XLaw = A_LAW
# NumTxTimeSlots, NumRxTimeSlots may be 16 or 32
DSP.C5x[0..1].NumTxTimeSlots = 16
DSP.C5x[0..1].NumRxTimeSlots = 16
DSP.C5x[0..1].CmdQStart = 0xE800
DSP.C5x[0..1].DataInQStart = 0xF800
DSP.C5x[0..1].DspOutQStart = 0xFB00
# The following is required when #timeslots = 32 (but not for 16)
#DSP.C5x[0..1].CmdQSize = 0x110
DSP.C5x[0..1].Libs[1] = cg6mslib
DSP.C5x[0].Files = cgcnfm
DSP.C5x[1].Files = cgcnfs
SwitchConnectMode = AllConstantDelay
ConferencingStream.Enable = YES
#---------------------------
# Resource management
#---------------------------
Resource[0].Name = RSC1
Resource[0].Size = 120
Resource[0].TCPs = nocc
Resource[0].StartTimeSlot = 0
################################################################
# Before modifying this resource definition string refer to the CG 6565
# Installation and Developers Manual.
# NOTE: echo.ln20_apt25 - echo running on DSP has been removed
# from resource definitions. We recommend user to use
# the hardware echo chip for echo cancellation instead
#################################################################
Resource[0].Definitions = ( dtmf.det_all & ptf.det_2f & tone.gen & \
callp.gnc & ptf.det_4f & \
( (rvoice.rec_mulaw & rvoice.play_mulaw) | \
(rvoice.rec_alaw & rvoice.play_alaw) | \
(rvoice.rec_lin & rvoice.play_lin) | \
(voice.rec_16 & (voice.play_16_100 | voice.play_16_150 | voice.play_16_200)) | \
(voice.rec_24 & (voice.play_24_100 | voice.play_24_150 | voice.play_24_200)) | \
(voice.rec_32 & (voice.play_32_100 | voice.play_32_150 | voice.play_32_200)) | \
(voice.rec_64 & (voice.play_64_100 | voice.play_64_150 | voice.play_64_200)) | \
(wave.rec_11_16b & wave.play_11_16b) | \
(wave.rec_11_8b & wave.play_11_8b) | \
(oki.rec_24 & (oki.play_24_100 | oki.play_24_150 | oki.play_24_200)) | \
(oki.rec_32 & (oki.play_32_100 | oki.play_32_150 | oki.play_32_200)) | \
(ima.rec_24 & ima.play_24) | \
(ima.rec_32 & ima.play_32) | \
(gsm_ms.frgsm_rec & gsm_ms.frgsm_play) | \
g726.rec_32 | g726.play_32) )
# NOTE: If the DSP cores listed below do not exist on the board, the DSP cores will
# be ignored and will not be booted or used
Resource[0].Dsps = 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 \
24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 \
43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 \
62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 \
81 82 83 84 85 86 87 88 89 90 91 92 93 94 95
DebugMask = 0x0