# Show switch connections: showcx95

Displays switch connections.

#### Usage

showcx95 [switch_driver]

#### Description

Displays the switch connections for all boards that have MVIP
switches. If a pattern is being sent on a timeslot
, the pattern value is displayed.

#### Procedure

To run showcx95 for AG boards, enter the following command:

showcx95 agsw

#### Example

The following example makes connections between an AG 2000 board and an AG 4040 board.

The following ppx.cfg file is used for this example:

[PPX]
Fabric
Bus H100
CTBUS:0..15:0..31
CTBUS:16..23:0..63
CTBUS:24..31:0..127
End Bus
Switch 0 ## AG 2000
SwitchType = HMIC
DeviceName = "agsw"
DeviceNumber = 0
Bus H100 (CTBUS:0..15:0..31)
Inputs
LOCAL:0..6(2):0..7
End Inputs
Outputs
LOCAL:1..7(2):0..7
End Outputs
End Switch
Switch 2 ## AG 4040
SwitchType = HMIC
DeviceName = "agsw"
DeviceNumber = 2
Bus H100 ()
Inputs
LOCAL:0..14(2):0..23 # Trunk
LOCAL:16..18(2):0..127 # DSP
End Inputs
Outputs
LOCAL:1..15(2):0..23 # Trunk
LOCAL:17..19(2):0..127 # DSP
End Outputs
End Switch
End Fabric

For the following swish commands:

ppx.Connect 0:local:0:0 to 2:local:17:0 SIMPLEX
ppx.Connect 0:local:0:2 to 2:local:17:2 DUPLEX
ppx.Connect 0:local:0:4 to 2:local:17:4 QUAD

The showcx95 output is:

SHOWCX95 Version 1.1 Jan 15 2004
AGSW 0
M-14:02 <- L-00:00
M-14:04 <- L-00:02
M-14:06 <- L-00:04
M-14:07 <- L-02:04
L-01:00 <- 0x7f
L-01:02 <- M-15:00
L-01:04 <- M-15:01
L-01:06 <- 0x7f
L-03:00 <- 0x00
L-03:02 <- 0x00
L-03:04 <- M-15:02
AGSW 2
M-15:00 <- L-16:02
M-15:01 <- L-16:04
M-15:02 <- L-18:04
L-01:00..23 <- 0x7f
[...]
L-15:00..23 <- 0x00
L-17:00 <- M-14:02
L-17:01 <- 0x7f
L-17:02 <- M-14:04
L-17:03 <- 0x7f
L-17:04 <- M-14:06
L-17:05..127 <- 0x7f
L-19:00..03 <- 0x00
L-19:04 <- M-14:07
L-19:05..127 <- 0x00

In the showcx95 output, M indicates MVIP bus and L indicates local bus. The showcx95 output shows three types of connections:

- Pattern 0x7F is sent to timeslot Local:01:02.

L-01:02 <- 0x7f

- Timeslots Local:00:00..04 are writing to timeslots Local:05:00..03.

L-05:00..03 <- L-00:00..04

- Timeslot MVIP:00:00 is writing to timeslot Local:01:00.
  Timeslot Local:00:00 is writing to timeslot MVIP:01:00 (a duplex connection).

M{00/01}:00 <-> L{01/00}:00