# ETSI (France) caller ID data

The following table describes the caller ID format for ETSI (France):

Parameter | Values | Type | Length | Field
Calling line number | Calling number identity | 0x02 | up to 30 up to 20 | Receive: NCC_CALL_STATUS.callingaddr Send: nccPlaceCall (callingaddr)
Reason for absence of number | O - Unavailable P - Private | 0x04 | 1 | Receive: NCC_CAS_EXT_CALL_STATUS.ANIpresentation Send: CAS_PLACECALL_EXT.ANIpresentation
Calling name | Calling name | 0x07 | up to 30 up to 31 | Receive: NCC_CALL_STATUS.callingname Send: CAS_PLACECALL_EXT.callingname
Reason for absence of name | O - Unavailable P - Private | 0x08 | 1 | Receive: NCC_CAS_EXT_CALL_STATUS.NAMEpresentation Send: CAS_PLACECALL_EXT.ANIpresentation
Called number (DDN) | Dialed number or dialable directory number (DDN) | 0x03 | up to 30 up to 31 | Receive: NCC_CALL_STATUS.calledaddr Send: nccPlaceCall (calledaddr)
Type of forwarded call | 0x00 - Unavailable or unknown 0x01 - Forward on busy 0x02 - Forward on no reply 0x03 - Unconditional forward 0x04 - Deflected call (after alerting) 0x05 - Deflected call (immediate) 0x06 - Forward on inability to reach mobile subscriber | 0x15 | 1 | Receive: NCC_CAS_EXT_CALL_STATUS.redirectingreason Send: CAS_PLACECALL_EXT.redirectingreason
Type of user calling | 0x00 - Origination unknown or unavailable 0x01 - Voice 0x02 - Text 0x03 - VPN (virtual private network) 0x04 - Mobile phone 0x05 - Mobile phone + VPN 0x06 - Fax 0x07 - Video 0x08 - Email 0x09 - Operator 0x0A - Ordinary calling subscriber 0x0B - Calling subscriber with priority 0x0C - Data call 0x0D - Test call 0x0E - Telemetric call 0x0F - Pay phone | 0x16 | 1 | Receive: NCC_CAS_EXT_CALL_STATUS.usercategory Send: CAS_PLACECALL_EXT.usercategory
Redirecting number | Last redirecting party | 0x1A | up to 30 up to 20 | Receive: NCC_CAS_EXT_CALL_STATUS.redirectingaddr Send: CAS_PLACECALL_EXT.redirectingaddr
Call type | 0x01 - Voice 0x02 - Ringback when free 0x03 - Calling name delivery 0x04 - Call return 0x05 -Alarm 0x06 - Download function 0x07 - Reverse charge 0x10 - External 0x11 - Internal 0x50 - Monitoring 0x81 - Message waiting | 0x11 | 1 | Receive: NCC_CAS_EXT_CALL_STATUS.tollcategory Send: CAS_PLACECALL_EXT.tollcategory
Network operator extended information | CCCNNNNVVV Where: C = Country N = Network V = Version | 0xE0 | 10 | Receive: NCC_CAS_EXT_CALL_STATUS.carrierid Send: CAS_PLACECALL_EXT.carrierid
Visual indicator | Message waiting indicator | 0x0B | 1 | Receive: NCC_CAS_EXT_CALL_STATUS.MWIndicator Send: CAS_PLACECALL_EXT.MWIndicator
Date/time | MMDDhhmm | 0x01 | 8 | Receive: NCC_CAS_EXT_CALL_STATUS.datetime Send: CAS_PLACECALL_EXT.datetime