# Interfaces by board type

The following table provides an example of the interfaces used by the various Dialogic boards and servers:

Interface example | Interface | Board name
| RJ-45 Ethernet 10/100Base-T | CG 6060 CG 6060C TX 4000 TX 4000/20 TX 4000C TX 4000C/20 TX 5500E (for Ethernet redundancy) TX 5020E (for Ethernet redundancy)
| RJ-45 Ethernet 10/100/1000Base-T | CG 6565 CG 6565C (does not apply to PICMG 2.16 versions) CG 6565E TX 5500E (for IP/SIGTRAN) TX 5020E (for IP/SIGTRAN)
| RJ-48C | CG 6060 1 T/E CG 6060 2 T/E CG 6060C 4 T/E CG 6060C 8 T/E (not all variants) CG 6565E 1 T/E CG 6565E 2 T/E
| Dialogic® MD1 RJ-45 interface | CG 6060 4 T/E CG 6565 4 T/E CG 6565E 4 T/E TX 4000 TX 4000/20 TX 5500E TX 5020E Vision VoiceXML Server (VX 5000-8) Vision Media Gateway (VG-2000-4) Vision Signaling Server (TIGI2U)
| Dialogic® MD1 RJ-21 | CG 6060C 8 T/E (not all variants) CG 6060C 16 T/E CG 6565C 8 T/E CG 6565C 16 T/E MG 7000A 16 T/E TX 4000C TX 4000/20C
| Dialogic® MD1 Mini RJ-21 interface | CG 6565 8 T/E CG 6565E 8 T/E Vision Media Gateway (VG 2000-8)