# bpikwMode

Whether the Supervisor keyword is read-only or read/write.

#### Syntax

Integer { readOnly(1), readWrite(2) }

#### Access

Read-only

#### OID

p.2.1.1.6.n

#### Details

bpikwMode reflects the value of the keyword's ReadOnly qualifier in the NMS OAM database.

#### Configuration

When it starts up, the OAM Database SNMP agent populates all MIB tables based upon information from the NMS OAM database. For more information, refer to the OAM Board Plug-in table.