# Dialogic® MD1 RJ-45 to two BNC pairs splitter cable

The Dialogic® MD1 RJ-45 to two BNC pairs splitter cable (P/N 83232) divides the two trunks on one Dialogic® MD1 RJ-45 to two BNC adapters.

Some countries require different adapter cables. Dialogic offers a splitter cable with the shield connected to transmit and receive outer conductors:

Note: This cable does not convert impedance. To connect a CG board with Dialogic® MD1 RJ-45 interfaces to a 75-ohm connection, you must either use this cable and configure the board as G703_75_OHM, or use an external balun and configure the board for 120-ohm operation.