# IMGT_D_CHANNEL_STATUS_CO

Returned in response to a D channel status request, with an attached buffer containing an imgt_d_channel_status structure.

#### Related structure

struct imgt_d_channel_status
{
BYTE status; /* Status (Released/Established/
Awaiting Establishment) */
BYTE bpad[3];
};

Field | Description | 4 E S S | E 1 0 | N I 2 | D M S | E T S I | V N 6 | H K G | A U S T E L 1 | N T T | K O R E A | T A I W A N | Q S I G | D P N S S | T 1 6 0 7
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
status | D channel status: IMGT_D_CHANNEL_STATUS_RELEASED IMGT_D_CHANNEL_STATUS_ESTABLISHED IMGT_D_CHANNEL_STATUS_AWAITING | x | x | x | x | x | x | x | x | x | x | x | x |  | x

Note: E10 is the same variant as 5ESS.