# Location values

The following table lists the valid location values for ACU_ALERT_IN, ACU_ALERT_RQ, ACU_CALL_PROC_IN, ACU_CALL_PROC_RQ, ACU_CLEAR_IN, ACU_CONN_IN, ACU_CONN_RQ, ACU_PROGRESS_IN, ACU_PROGRESS_RQ, and ACU_SETUP_REPORT_IN messages.

These values are defined in isdnval.h.

Location | Description
--- | ---
LOC_USER (Default if partner_equip argument passed to isdnStartProtocol is EQUIPMENT_NT) | User.
LOC_PR_LOCAL_USER | Private network serving the local user.
LOC_NETWORK (Default if partner_equip argument passed to isdnStartProtocol is EQUIPMENT_TE) | Location network (SWD).
LOC_TRANSIT_NET | Transit network.
LOC_PU_REMOTE_USER | Public network serving the remote user.
LOC_PR_REMOTE_USER | Private network serving the remote user.
BEYOND_IWP (Default for DMS variant) | Network beyond interworking point.