# brdkwMode

If the board keyword is read-only or read-write.

#### Syntax

Integer { readOnly(1), readWrite(2) }

#### Access

Read-only

#### OID

p.4.3.1.6.n

#### Details

brdkwMode reflects the value of the keyword's ReadOnly qualifier in the NMS OAM database.

#### Configuration

When it starts up, the OAM Database SNMP agent populates all MIB tables based upon information from the NMS OAM database. For more information, see OAM Boards table.