# ADI_FSKSEND_PARMS

#### Dependent function: adiStartSendingFSK

Field name | Type | Default | Units | Description
--- | --- | --- | --- | ---
baudrate | DWORD | 1200 | integer | Transmission baud rate. 1200 is the only valid value.
level | INT32 | -14 | dBm | Transmit output level.
marktime | DWORD | 500 | ms | Length of initial mark signal.
noseizureflag | DWORD | 1 | integer | Controls whether channel seizure is omitted. 0 = send channel seizure 1 = just send mark
seizetime | DWORD | 1000 | ms | Duration of channel seizure; ignored if noseizureflag = 1.