# NCC.X.ADI_PLACECALL

Dependent function: nccPlaceCall

Note: All Field names in this structure are prefaced with NCC.X.ADI_PLACECALL; for example, NCC.X.ADI_PLACECALL.mediamask.

Field name | Type | Default | Units | Description
--- | --- | --- | --- | ---
connectmask | DWORD | 0x0103 | mask | Determines how an outbound call gets connected. Valid values are: 0x0001: Connect on out of band signal. 0x0002: Connect on call progress (cp) beginning of voice. 0x0004: Connect on call progress medium length voice detected. 0x0008: Connect on call progress long voice. 0x0010: Connect on call progress extended voice. 0x0020: Connect on call progress voice end. 0x0080: Connect on call progress ring stopping. 0x0100: Connect on call progress CED detected. 0x0200: Connect on call progress dial tone detected. 0x0400: Connect on call progress SIT tone detected. 0x0800: Connect on call progress ring begin. 0x8000: Do not run call progress.
disconnectmask | DWORD | 0x0040 | mask | Determines how to abandon an outgoing call. Valid values are: 0x0002: Disconnect on call progress (cp) beginning of voice. 0x0004: Disconnect on call progress medium voice detected. 0x0008: Disconnect on call progress long voice detected. 0x0010: Disconnect on call progress extended voice detected. 0x0020: Disconnect on call progress voice ended. 0x0040: Disconnect on call progress timeout. 0x0080: Disconnect on call progress ring tone stopped. 0x0100: Disconnect on call progress CED tone detected. 0x0800: Disconnect on call progress ring begin.
callprog.timeout | DWORD | 1000 | ms | Maximum time that can elapse with no stimulus from the network before call progress stops with a reason of timeout. Valid range is 1 through 65535. If the value is set to zero, the timer is disabled.
callprog.busycount | DWORD | 4 | count | Number of non-precise busy tones that must occur before busy or fast busy is reported. Valid range is 1 through 32767.
callprog.ringcount | DWORD | 7 | count | Number of ring tones that must occur before NO_ANSWER is reported. Valid range is 1 through 32767.
callprog.maxreorder | DWORD | 700 | ms | Threshold time defining the total time period (on time plus off time) for distinguishing between fast busy (reorder) and slow busy. Valid range is 0 through 32767.
callprog.maxbusy | DWORD | 1500 | ms | Threshold time defining the total time period (on time plus off time) for distinguishing between slow busy and ringing tone. Valid range is 0 through 32767.
callprog.maxring | DWORD | 3000 | ms | Maximum duration of a tone to distinguish a ringing tone from a dial tone. Valid range is 0 through 32767.
callprog.maxringperiod | DWORD | 8000 | ms | Length of time of the last ringing tone plus the silence that follows, before call progress reports a ringing-ended event.
callprog.voicemedium | DWORD | 3000 | ms | Minimum length of time voice must be detected before call progress reports a medium-voice event.
callprog.voicelong | DWORD | 6000 | ms | Minimum length of time voice must be detected before call progress reports a long-voice event.
callprog.voicextended | DWORD | 9000 | ms | Minimum length of time voice must be detected before call progress reports an extended-voice event.
callprog.silencetime | DWORD | 1500 | ms | Minimum length of a silent period after voice is detected before call progress reports a voice-ended event.
callprog.precqualtime | DWORD | 150 | ms | Precise tone qualification time. All precise tones must be longer than this time to qualify.
callprog.precmask | DWORD | 7 | mask | Mask to control which precise detectors to run. Form a value by using the OR operator with any of the following bit masks: NCC_CPMSK_PRECISE_CED (0x0001): CED tone modem NCC_CPMSK_PRECISE_SIT (0x0002): SIT NCC_CPMSK_PRECISE_BUSY (0x0004): Busy and reorder tone (US) NCC_CPMSK_PRECISE_425 (0x0008) 425 Hz tone (busy and reorder tone, non-US) NCC_CPMSK_PRECISE_SITEXT (0x0010): SIT type reporting NCC_CPMSK_PRECISE_TDD (0x0020): TDD/TTY device NCC_CPMSK_PRECISE_NU (0x0040): Unassigned number Only three of the four detectors can run concurrently. If all four detectors are specified, busy and reorder tones are determined by cadence alone. The SIT, CED, and TDD/TTY detectors are enabled. Busy and reorder tone (bit value 0x0004) and the 425 Hz tone selection (bit value 0x0008) are mutually exclusive. If you choose both, only the 425 Hz filter takes effect.
callprog.stopmask | DWORD | 0 | mask | Mask to control which events cause call progress to stop. A value can be formed by using the OR operation with any of the following values: 0x0001: Ring tone 0x0002: Ring end 0x0004: Voice begin 0x0008: Medium voice duration 0x0010: Long voice duration 0x0020: Extended voice duration 0x0040: Voice end
callprog.silencelevel | INT32 | -40 | dBm | Maximum signal level that is considered to be silence. Valid AG board and CG board range is -46 through -34. Valid QX board range is -45 through 0.
callprog.voicetoneratio | DWORD | 0x30000 | IDU | Do not modify.
callprog.qualtonetime1 | DWORD | 60 | ms | Do not modify.
callprog.qualtonetime2 | DWORD | 80 | ms | Do not modify.
callprog.qualvoicetime1 | DWORD | 60 | ms | Do not modify.
callprog.qualvoicetime2 | DWORD | 60 | ms | Do not modify.
callprog.leakagetime | DWORD | 8 | ms | Do not modify.
callprog.noiselevel | DWORD | 0x14000 | IDU | Do not modify.