# Retrieving AG board configuration information: boardinf

boardinf is a program that reports the board number, address, type, number of ports, memory, and DSP timeslot assignments for each AG board in a system.

boardinf opens the AG driver and retrieves the configuration information for up to 16 AG 2000C boards. If an AG 2000C board exists and is properly initialized, its configuration is displayed and its DSP port addresses are displayed as one or more timeslot ranges.

To run boardinf:

Step | Action
1 | Ensure that the AG 2000C boards were initialized.
2 | Open a command window.
3 | Enter the following command: boardinf boardinf displays the configuration information for each AG 2000C board in the system that has been loaded and initialized.
4 | If no boards are detected, verify that the AG 2000C board(s) is loaded and initialized and repeat the command. If the AG 2000C configuration information is not as expected, review the board keyword file.