# brdkwAllowedRange

Range of allowed values for the board keyword.

#### Syntax

DisplayString (SIZE 0..255)

#### Access

Read-only

#### OID

p.4.3.1.7.n

#### Details

If the keyword type is integer, and is a yes or no choice, brdkwAllowedRange contains a string in this format:

Nb values=2: Yes,No

If the keyword type is integer, and can take a range of values, brdkwAllowedRange contains a string in this format:

BASE base:min_value <> max_value

Where:

- base is a mathematical base of the integer (for example, 16 for a hexadecimal number).

- min_value is the minimum allowed value.

- max_value is the maximum allowed value.

For example:

BASE 10: 0 <> 65535

If the keyword type is string, brdkwAllowedRange contains all the allowed strings for this keyword, separated by commas (,). For example: YES,NO. If any string is acceptable, this field contains <no range>.

brdkwAllowedRange reflects the combined values of the Base, Min, Max, and Choices qualifiers for the keyword in the NMS OAM database.

#### Configuration

When it starts up, the OAM Database SNMP agent populates all MIB tables based upon information from the NMS OAM database. For more information, see OAM Boards table.