# EL7 parameters

The following table describes NCC.X.ADI_EL7 parameters. Generally, these parameters are not altered from their default values.

Field | Unit | Default | Description
--- | --- | --- | ---
WaitForPC | ms | 10000 | Time protocol will wait for application before taking independent action.
WaitForSeizureAck | ms | 5000 | (0 = forever) waiting for network acknowledgment of the seizure (outbound).
WaitForAnswerAck | ms | 2000 | (0 = forever) waiting for network acknowledgment after answering call (inbound).
WaitBeforeOutOfService | ms | 25000 | (0 = forever) waiting for network idle before line is taken out of service.
QualifyOn | ms | 12 | Qualification of signaling detector changes (DSP).
PulseIn | ms | 25 | Qualification of received detector changes (TCP).
PulseOut | ms | 60 | Duration of transmitted signaling pulses.
WaitIdleAfterReject | ms | 120 | After rejecting inbound call, time before idle.
WaitForReconnectBack | ms | 2000 | Wait for recall after clearing second call.
WaitForRecallAck | ms | 5000 | Wait for recall register acknowledge.
ReleaseGuard | ms | 650 | Minimum idle time after call clearing.
NetworkSide | mask | 0 | Must be set to 0.
WaitForAnswerOffHook | ms | 20000 | Do not modify.
VariableDigits | ms | 1 | Do not modify.
NumberOfDigits | count | 3 | Do not modify.
WaitFirstDigit | ms | 7000 | Do not modify.
WaitNextDigit | ms | 3000 | Do not modify.