# NCC service global parameters

This topic describes the following NCC implementation-independent, protocol-independent parameters, defined in nccstart.pf:

- NCC.START structure

- NCC.START.callproggenerate parameters

- NCC.START.eventmask bits

The parameters are alphabetized by category and subcategories. Within each category, fields are listed alphabetically. For information on implementation-dependent or protocol-dependent parameters, see your protocol-specific documentation.

## NCC.START structure

NCC.START
Dependent Function(s): nccStartProtocol
Field name | Type | Default | Units | Description
--- | --- | --- | --- | ---
eventmask | DWORD | 0x0000 | mask | Determines which events are sent to the application.
debugflag | WORD | 0 | integer | Reports low-level debug events to the application. Off (0) or on (non-zero).
waitforPCtime | WORD | 10000 | ms | Specifies the time to wait for the application to respond after an NCCEVN_INCOMING_CALL. If a response is not received within the timeout, the incoming call is rejected.
overlappedreceiving | WORD | 0 | integer | Determines if the protocol will receive digits in overlapped receiving mode.

## NCC.START.callproggenerate parameters

NCC.START.callproggenerate
Dependent function(s): nccStartProtocol
Field name | Type | Default | Units | Description
--- | --- | --- | --- | ---
dialtonefreq1 | WORD | 350 | Hz | First frequency of dialtone.
dialtonefreq2 | WORD | 440 | Hz | Second frequency of dialtone.
dialtoneontime1 | WORD | -1 | ms | Cadenced dialtone: first ON time.
dialtoneontime2 | WORD | 0 | ms | Cadenced dialtone: second ON time.
dialtoneofftime1 | WORD | 0 | ms | Cadenced dialtone: first OFF time.
dialtoneofftime2 | WORD | 0 | ms | Cadenced dialtone: second OFF time.
dialtonelevel | WORD | 150 | IDU | Dialtone amplitude.
ringfreq1 | WORD | 440 | Hz | First frequency of ringback tone.
ringfreq2 | WORD | 480 | Hz | Second frequency of ringback tone.
ringontime | WORD | 1000 | ms | Ringback tone ON time.
ringofftime1 | WORD | 3000 | ms | Ringback tone first (or only) OFF time.
ringofftime2 | WORD | 0 | ms | Ringback tone second OFF time.
ringtonelevel | WORD | 112 | IDU | Ringback tone amplitude.
busyfreq1 | WORD | 480 | Hz | First frequency of busy tone.
busyfreq2 | WORD | 620 | Hz | Second frequency of busy tone.
busyontime | WORD | 500 | ms | Busy tone ON time.
busyofftime | WORD | 500 | ms | Busy tone OFF time.
busytonelevel | WORD | 63 | Hz | Busy tone amplitude.
fastbusyfreq1 | WORD | 480 | Hz | First frequency of fast busy (reorder) tone.
fastbusyfreq2 | WORD | 620 | Hz | Second frequency of fast busy (reorder) tone.
fastbusyontime | WORD | 250 | ms | Fast busy tone ON time.
fastbusyofftime | WORD | 250 | ms | Fast busy tone OFF time.
fastbusytonelevel | WORD | 63 | IDU | Fast busy tone amplitude.

## NCC.START.eventmask bits

The NCC.START.eventmask parameter controls which events are returned to the application. The following table lists the eventmask bits and the events they control:

Value | Bit name | Event reported
--- | --- | ---
0x4 | NCC_REPORT_ALERTING | NCCEVN_REMOTE_ALERTING
0x8 | NCC_REPORT_ANSWERED | NCCEVN_REMOTE_ANSWERED
0x20 | NCC_REPORT_BILLING | NCCEVN_BILLING_INDICATION
0x40 | NCC_REPORT_STATUSINFO | NCCEVN_CALL_STATUS_UPDATE NCCEVN_EXTENDED_CALL_STATUS_UPDATE
0x10000 | NCC_REPORT_CALLID | NCCEVN_CALLID_AVAILABLE