# ADI_CALLPROG_PARMS

#### Dependent function: adiStartCallProgress

Field name | Type | Default | Units | Description
--- | --- | --- | --- | ---
busycount | DWORD | 4 | count | Number of non-precise busy tones that must occur before busy or fast busy is reported. Valid range is 1 through 32767.
leakagetime | DWORD | 8 | ms | Do not modify.
maxbusy | DWORD | 1500 | ms | Threshold time defining the total time period (on time plus off time) for distinguishing between slow busy and ringing tone. Valid range is 0 through 32767.
maxreorder | DWORD | 700 | ms | Threshold time defining the total time period (on time plus off time) for distinguishing between fast busy (reorder) and slow busy. Valid range is 0 through 32767.
maxring | DWORD | 3000 | ms | Maximum duration of a tone to distinguish a ringing tone from a dial tone. Valid range is 0 through 32767.
maxringperiod | DWORD | 8000 | ms | Length of time of the last ringing tone plus the silence that follows, before call progress reports a ringing-ended event.
noiselevel | DWORD | 0x14000 | IDU | Do not modify.
precmask | DWORD | 7 | mask | Mask to control which precise detectors to run. Use the OR operator with any of the following bit masks to form a value: ADI_CPMSK_PRECISE_CED (0x0001): CED tone modem ADI_CPMSK_PRECISE_SIT (0x0002): SIT ADI_CPMSK_PRECISE_BUSY (0x0004): Busy and reorder tone (US) ADI_CPMSK_PRECISE_425 (0x0008) 425 Hz tone (busy and reorder tone, non-US) ADI_CPMSK_PRECISE_SITEXT (0x0010): SIT type reporting ADI_CPMSK_PRECISE_TDD (0x0020): TDD/TTY device ADI_CPMSK_PRECISE_NU (0x0040): Unassigned number You can run three of the four detectors concurrently. If you specify all four detectors, busy and reorder tones are determined by cadence alone, and only the SIT, CED, and TDD/TTY detectors are enabled. Busy and reorder tone (bit value 0x0004) and the 425 Hz tone selection (bit value 0x0008) are mutually exclusive. If you choose both, only the 425 Hz filter is in effect.
precqualtime | DWORD | 150 | ms | Precise tone qualification time. All precise tones must be longer than this time to qualify.
qualtonetime1 | DWORD | 60 | ms | Do not modify.
qualtonetime2 | DWORD | 80 | ms | Do not modify.
qualvoicetime1 | DWORD | 60 | ms | Do not modify.
qualvoicetime2 | DWORD | 60 | ms | Do not modify.
ringcount | DWORD | 7 | count | Number of ring tones that must occur before NO_ANSWER is reported. Valid range is 1 through 32767.
silencelevel | INT32 | -40 | dBm | Maximum signal level that is considered to be silence. Valid AG board and CG board range is -46 through -34.
silencetime | DWORD | 1500 | ms | Minimum length of a silent period after voice is detected before call progress reports a voice-ended event.
stopmask | DWORD | 0 | mask | Mask to control which events cause call progress to stop. A value can be formed by using the OR operation with any of the following values: 0x0001 = ring tone 0x0002 = ring end 0x0004 = voice begin 0x0008 = medium voice duration 0x0010 = long voice duration 0x0020 = extended voice duration 0x0040 = voice end
timeout | DWORD | 1000 | ms | Maximum time that can elapse with no stimulus from the network before call progress stops with reason of timeout. Valid range is 1 through 65535. If the value is set to zero, the timer is disabled.
voicextended | DWORD | 9000 | ms | Minimum length of time voice must be detected before call progress reports an extended-voice event.
voicelong | DWORD | 6000 | ms | Minimum length of time voice must be detected before call progress reports a long-voice event.
voicemedium | DWORD | 3000 | ms | Minimum length of time voice must be detected before call progress reports a medium-voice event.
voicetoneratio | DWORD | 0x30000 | IDU | Do not modify.