# CG 6060 board features

The CG 6060 board is a Dialogic PCI media board. It is a high-density platform for IVR, fax, VoIP, and media server applications. The board uses a high performance PowerPC processor.

Configurations support up to four T1 or E1 digital trunk interfaces and up to two Ethernet 10/100Base-T interfaces.

Refer to the www.dialogic.com/declarations/default.htm for a list of available CG 6060 board configurations, for a list of countries where Dialogic has obtained approval for the CG 6060 board, and for product updates.

CG 6060 boards include the following features:

- DSP resources

  The CG 6060 board has up to 4256 MIPS of media processing DSPs.

- PCI bus connectivity

  Each CG 6060 board is designed to reside in a single PCI bus slot. Each board contains a universal (5 V or 3.3 V signaling) PCI bus interface compliant with the PCI Local Bus Specification, Revision 2.2. The PCI interface is a 33 or 66 MHz 32-bit device.

- Trunk connectivity

  Board configurations provide up to four T1 or E1 network interfaces for digital trunk connectivity. You must configure the board for either T1 or E1. For more information, refer to Configuring the T1 or E1 interface and to NetworkInterface.T1E1[x].Type.

- H.100 bus connectivity

  The CG 6060 board fully supports the H.100 bus specification. The H.100 bus enables multiple boards to share data. For example, you can connect two or more CG 6060 boards for applications that perform trunk-to-trunk switching. You can use H.100 compatible products from other manufacturers with the CG 6060 board.

  The H.100 interface supports the following stream configurations on the H.100 bus:

  - Full mode: 32 streams at 8 MHz each, which provides 128 timeslots each for a total of 4096 timeslots.

  - Backward compatibility mode: 16 8-MHz streams, 16 2-MHz streams (total of 2560 timeslots). The H.100 interface can operate with MVIP-90 boards on the same bus. In this configuration, an H.100 board in the system must be the bus master.

- Telephony bus switching

  Switching for the CG 6060 board offers support for the H.100 bus within the H.100 architecture. On the CG 6060 board, switch connections are allowed for a total of 512 full duplex connections between local devices and the H.100 bus.

- Ethernet connectivity

  The CG 6060 board contains two 10/100Base-T Ethernet connections for fast Ethernet connectivity and support of both IPv4 and IPv6. For more information, refer to Connecting to an Ethernet network.

- Echo cancellation

  CG 6060 boards support up to 120 ports of line echo cancellation with 64 ms tails.

The following illustration shows where various components are located on a CG 6060 board: