# NCC.X.ADI_START.dial

The following table describes NCC.X.ADI_START.dial parameters:

NCC.X.ADI_START.dial
Dependent functions: nccStartProtocol
Field | Type | Default | Units | Description
--- | --- | --- | --- | ---
breaktime | DWORD | 60 | ms | Break (on-hook) duration for dial pulses. Valid AG and CG range is 0 to 30000. Valid QX range is 0 to 32767.
dialtonewait | DWORD | 5000 | ms | Maximum time to wait for dial tone (applies only to the semicolon (;) character). Valid range is 0 to 65535.
dtmfampl1 | INT32 | -6 | dBm | Amplitude of the low frequency component of the DTMF pair. Valid AG and CG range is -54 to -3. Valid QX range is -90 to 0.
dtmfampl2 | INT32 | -4 | dBm | Amplitude of the high frequency component of the DTMF pair. Valid AG and CG range is -54 to -3. Valid QX range is -90 to 0.
dtmfofftime | DWORD | 80 | ms | Duration of the silence time between each digit. Valid AG and CG range is 0 to 65534. Valid QX range is 0 to 2047.
dtmfontime | DWORD | 80 | ms | Duration of each DTMF or MF digit. Valid AG and CG range is 0 to 65534. Valid QX range is 0 to 2047.
flashtime | DWORD | 500 | ms | Amount of time to assert the on-hook signaling pattern for a flash (!) character. Valid AG and CG range is 0 to 65535. Valid QX range is 0 to 32767.
interpulse | DWORD | 700 | ms | Inter-digit time for pulsed dialing. Valid AG and CG range is 0 to 30000. Valid QX range is 0 to 32767.
longpause | DWORD | 5000 | ms | Amount of delay associated with the period (.) character. Valid range is 0 to 65535.
maketime | DWORD | 40 | ms | Make (off-hook) duration for dial pulses. Valid AG and CG range is 0 to 30000. Valid QX range is 0 to 32767.
method | DWORD | 0 | mask | Type of signaling: 0=DTMF, 1=Pulse, 2=MF (US).
reserved | DWORD | 0 | internal | Do not modify.
shortpause | DWORD | 2000 | ms | Amount of delay associated with the comma (,) character. Valid range is 0 to 65535.
tonebandw1 | DWORD | 40 | Hz | Bandwidth of the first frequency of the dial tone detector. Valid AG and CG range is 20 to 800. Valid QX range is 40 to 2000.
tonebandw2 | DWORD | 40 | Hz | Bandwidth of the second frequency of the dial tone detector. Valid AG and CG range is 20 to 800. Valid QX range is 40 to 2000.
tonefreq1 | DWORD | 350 | Hz | First (or only) dial tone frequency. Valid AG and CG range is 330 to 3600. Valid QX range is 1 to 4000.
tonefreq2 | DWORD | 440 | Hz | Second dial tone frequency. Set this to 0 to detect a single frequency. Valid AG and CG range is 330 to 3600. Valid QX range is 1 to 4000.
tonequalampl | INT32 | -28 | dBm | Minimum broadband signal amplitude to qualify for dial tone detection. Valid AG and CG range is -40 to 0. Valid QX range is -48 to 0.
tonequaltime | DWORD | 50 | ms | Minimum duration of a qualified tone to be considered dial tone. Valid range is 0 to 32767.
tonereflevel | DWORD | 0xb000 | IDU | Do not modify.
tonetotaltime | DWORD | 0 | ms | Total time interrupted dialtone must be present.