# SwitchConnections

Specifies whether the board nails up default switch connections when initialized.

#### Syntax

SwitchConnections = mode

#### Access

Read/Write

#### Type

String

#### Default

AUTO

#### Allowed values

YES | NO | AUTO

#### Example

SwitchConnections = No

#### Details

Valid entries include:

Value | Description
--- | ---
YES | Nails up switch connections regardless of the Clocking.HBus.ClockMode keyword setting.
NO | Does not nail up switch connections.
AUTO | Nails up connections automatically if the Clocking.HBus.ClockMode keyword is set to STANDALONE.

When running the Point-to-Point Switching service
, set SwitchConnections = NO. Use the ppx.cfg file to define default connections. For more information, refer to the Dialogic® NaturalAccess™ Point-to-Point Switching API Developer's Manual.

#### See also

SwitchConnectMode