# TempSensor[x].CritThres

Specifies the critical threshold of a temperature sensor in tenth of a degree Celsius.

#### Syntax

TempSensor[x].CritThres = temperature

x = 0 (index of the main temperature sensor)

x = 1 (index of the PPC temperature sensor)

x = 2 (index of the DSP temperature sensor)

x = 3 (index of the daughterboard temperature sensor)

#### Access

Read/Write

#### Type

Integer

#### Default

Main temperature sensor = 950

PPC temperature sensor = 1000

DSP temperature sensor =750

Daughterboard temperature sensor = 750

#### Allowed values

100 - 1200

#### Example

TempSensor[0].CritThres = 750

#### Details

The critical threshold temperature must be below the shutdown temperature or an OAM event will not be received. The following table lists the shutdown temperatures for the sensors on the board:

Sensor | Shutdown temperature
Main board | 105 °C
PPC | 105 °C
DSP | 85 °C
Daughterboard | 85 °C

#### See also

TempSensor[x].WarnThres