# cg6ktool - Displaying EEPROM and RAM

Displays EEPROM contents and dumps the on-board error log.

#### Usage

cg6ktool options

where options are:

Options | Description
--- | ---
-A | Lists the board's bus and slot information.
-B -lbus:slot | Blinks the board's LED.
-R -lbus:slot | Resets a specified board.
-M -lbus:slot -aaddress -ssize | Dumps memory in binary format to the file memdump_at_bus_slot.txt. If the starting byte (address) and number of bytes (size) are not specified, the defaults are 0 and 1 MB respectively. To dump the file in ASCII format, add the -t1 option.
-tfiletype | Specifies the file type (text = 1, binary = 2).
-S -lbus:slot | Dumps error and stack information to the file errdump_at_bus_slot.txt.
-eboarddeviceID | Applies the specified command to all CG boards of the specified type in the chassis. Can be used instead of -lbus:slot.
CG board type | Device ID
CG 6000 | 6003
CG 6000C | 6000
CG 6060 | 6060
CG 6060C | 6061
CG 6100C | 6100
CG 6500C | 6500
CG 6565 | 6565
CG 6565C | 6566
CG 6565E | 6568
-h | Displays help information.

An option applies to all boards if you do not specify either -l or -e.

cg6ktool supports multiple CG boards. Some of these commands are shown for reference only and may not pertain to the CG 6060C board.