# Show switch connections: showcx95

Displays switch connections.

#### Usage

showcx95 [-@server][-bboard_number][driver_name...]

where driver_name is the name of the switching driver for the board you are querying. The following table lists options for using this command:

This command... | Queries...
--- | ---
showcx95 | All boards in the system and displays the switch connections.
showcx95 driver_name | Boards with the given switching driver and displays the switch connections.
showcx95 -bboard_number | The indicated board or boards and displays the switch connections.
showcx95 -@server | All boards in the system specified by the server name or IP address. Default = localhost.

#### Description

showcx95 displays the switch connections for all boards that have MVIP switches. If a pattern is being sent on a timeslot
, the pattern value is displayed.

#### Example

If you have an AG board configured as board 0 with trunk channel 1 connected to local DSP
resources (both voice and signaling) and you run the following commands in swish:

SWISH: openswitch ag = agsw 0
SWISH: resetswitch ag
SWISH: makeconnection ag local:0:4..7 to local:5:0..3
SWISH: makeconnection ag mvip:0:0 to local:1:0 duplex

The output displays as:

SHOWCX95 Version 1.1 Jan 15 1998
AGSW 0
M{00/01}:00 <-> L{01/00}:00
L-01:02 <- 0x7f
L-01:04..07 <- 0x7f
L-03:00 <- 0x00
L-03:02 <- 0x00
L-03:04..07 <- 0x00
L-05:00..03 <- L-00:00..04
L-05:04..07 <- 0x7f
L-07:00..07 <- 0x00

In this output example, M means MVIP bus and L means local bus.

####

This output example shows these types of connections:

L-01:02 <- 0x7f

Pattern 0x7f is sent to timeslot Local:01:02.

L-05:00..03 <- L-00:00..04

Timeslots Local:00:00..04 are writing to timeslots Local:05:00..03.

M{00/01}:00 <-> L{01/00}:00

Timeslot MVIP:00:00 is writing to timeslot Local:01:00.
Timeslot Local:00:00 is writing to timeslot MVIP:01:00 (a duplex connection).

The syntax of showcx95 v1.1 for duplex connections is:

L|M{fwd slot1/rev slot1} <-> L|M{fwd slot2/rev slot2}

that represents fwd slot1 -> fwd slot2 and rev slot1 <- rev slot2.