# oamBoardGetBusSlot

Returns the PCI bus and slot number for a specified board. For more information, see Retrieving board information.

#### Prototype

DWORD oamBoardGetBusSlot ( CTAHD ctahd, const char *szName, DWORD *pdwBus, DWORD *pdwSlot )

Argument | Description
ctahd | [in] Context handle
szName | [in] Pointer to a name of board to look up.
pdwBus | [out] Pointer to the board's PCI bus number.
pdwSlot | [out] Pointer to the board's slot number.

#### Return values

Return value | Description
SUCCESS |
CTAERR_BAD_ARGUMENT | szName, pdwBus, or pdwSlot is NULL or 0.
CTAERR_SVR_COMM | Natural Access Server is not running.
OAMERR_NOT_FOUND | Board not found.
OAMERR_SERVER_NOT_RUNNING | Supervisor is shut down.

#### See also

oamBoardGetDriverIDs, oamBoardGetMACAddress, oamBoardGetNumber, oamBoardGetProduct, oamBoardGetSerialNumber, oamBoardGetShelfSlot, oamBoardGetStatus