# Board configuration: boardinf

Retrieves and displays the hardware and MVIP configuration for all boards that use Natural Access in the host computer.

#### Usage

boardinf

There are no command-line options.

#### Featured functions

adiGetBoardInfo, adiGetBoardSlots

#### Description

boardinf opens a board driver under the Natural Access environment and retrieves up to 16 board configurations. The program displays the configuration and a list of available DSP timeslots for each board, formatting this array into timeslot ranges before displaying it.

#### Procedure

Ensure that you have initialized the boards using the configuration utility.

Run boardinf by entering boardinf at the prompt.

Note: You can use adiGetBoardInfo and adiGetBoardSlots to retrieve system configuration information when initializing your applications.