# NetworkInterface.Analog[x].ConfigFile

Specifies the country-specific file for line interfaces for AG 2000 boards. Refer to QSLAC files and trunk control programs for more information.

#### Syntax

NetworkInterface.Analog[x].ConfigFile = filename

#### Access

Read/Write

#### Type

File name

#### Default

Line interface type | File name | Where used
--- | --- | ---
Loop start | a2usals6.slc | Default. Loop start for 600 Ohm PBXs in North America and South America.
| a2canls6.slc | Loop start for 600 Ohm PBXs in Canada.
| a2jpnls6.slc | Loop start for 600 Ohm PBXs in Japan.
| a2usals9.slc | Loop start for 900 Ohm PBXs in North America and South America.
| a2canls9.slc | Loop start for 900 Ohm PBXs in Canada.
| a2jpnls9.slc | Loop start for 900 Ohm PBXs in Japan.
| a2usalsn.slc | PSTN connections in North America and South America.
| a2canlsn.slc | PSTN connections in Canada.
| a2jpnlsn.slc | PSTN connections in Japan.
| a2eurlsc.slc | PSTN connections in the EU countries.
| a2auslsc.slc | PSTN connections for Australia.
Subscriber loop | a2usasl6.slc | Default subscriber loop interface.
| a2usasl9.slc | 900 Ohm subscriber loop interface.
DID | a2usadd6.slc | Default DID interface.
| a2usadd9.slc | 900 Ohm DID interface.

#### Allowed values

Valid QSLAC file name.

#### Example

NetworkInterface.Analog[x].ConfigFile = a2usals9.slc