# Dialogic® Hardware Connectivity Manual

The Dialogic® Hardware Connectivity Manual is written for those who plan and install solutions that contain CG Series Media Boards, TX Series SS7 Boards, and the Vision™ Family of Servers and Gateways.

This manual provides detailed information about connectors and connector pin assignments (interfaces) on Dialogic products, and defines the Dialogic signal entry panel (SEP) solutions used to convert products with Dialogic® MD1 RJ-21 interface and Dialogic® MD1 Mini RJ-21 interfaces to industry-standard RJ-48C Telco interfaces.

Warning: | Important safety notes for telephony connections Allow only qualified technical personnel to install NMS hardware and its associated telephone wiring. Make sure the PC chassis is grounded through the power cord or by other means before connecting the telephone line. If your system requires an external power supply, make sure it is grounded through the power cord or by other means. Never install telephone wiring during a lightning storm. Never install telephone jacks in wet locations. Telephone companies provide primary lightning protection for their telephone lines. However, if a site connects to private lines that leave the building, make sure that external protection is provided.

Revision history | © Copyright 2009 Dialogic Corporation. All rights reserved. | Notices