# PRI mode switching

This topic contains the following PRI mode switching information:

- PRI mode switch model

- H.110 and local streams

- Voice information routing on T1 trunks

- Voice information routing on E1 trunks

- T1/E1 signaling information routing

- Default connections

## PRI mode switch model

The following illustration shows the CG 6060C switching model in PRI
mode:

## H.110 and local streams

The following tables list the specific use of each stream
in the CG 6060C PRI switch model:

### H.110 streams

H.110 bus | Streams 0..31, timeslots 0..127 (Streams clocked at 8 MHz)

### Local streams

Trunk voice information (T1 trunks) | Trunk 1: Streams 0 and 1, Trunk 2: Streams 4 and 5, Trunk 3: Streams 8 and 9, Trunk 4: Streams 12 and 13, Trunk 5: Streams 16 and 17, Trunk 6: Streams 20 and 21, Trunk 7: Streams 24 and 25, Trunk 8: Streams 28 and 29, Trunk 9: Streams 32 and 33, Trunk 10: Streams 36 and 37, Trunk 11: Streams 40 and 41, Trunk 12: Streams 44 and 45, Trunk 13: Streams 48 and 49, Trunk 14: Streams 52 and 53, Trunk 15: Streams 56 and 57, Trunk 16: Streams 60 and 61, | timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22 timeslots 0..22
Trunk voice information (E1 trunks) | Trunk 1: Streams 0 and 1, Trunk 2: Streams 4 and 5, Trunk 3: Streams 8 and 9, Trunk 4: Streams 12 and 13, Trunk 5: Streams 16 and 17, Trunk 6: Streams 20 and 21, Trunk 7: Streams 24 and 25, Trunk 8: Streams 28 and 29, Trunk 9: Streams 32 and 33, Trunk 10: Streams 36 and 37, Trunk 11: Streams 40 and 41, Trunk 12: Streams 44 and 45, Trunk 13: Streams 48 and 49, Trunk 14: Streams 52 and 53, Trunk 15: Streams 56 and 57, Trunk 16: Streams 60 and 61, | timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29 timeslots 0..29
DSP voice information (T1 and E1 trunks) | Streams 64 and 65, timeslots 0.. up to 899

In PRI mode, an internal HDLC
controller automatically terminates the D channel signaling.

## Voice information routing on T1 trunks (PRI mode)

If NetworkInterface.T1E1[x].SignalingType = PRI, signaling information is routed to accommodate the T1 ISDN common channel signaling configuration where voice information is transmitted in the first 23 channels. Each voice channel on the T1 trunk is placed in a corresponding timeslot
on the local bus in the following streams:

## Voice information routing on E1 trunks (PRI mode)

Regardless of the NetworkInterface.T1E1[x].SignalingType setting, the CG 6060C board routes the voice information by assigning E1 timeslots 1 through 15 to the local bus timeslots 0..14. E1 timeslots 17 through 31 are assigned to the local bus timeslots 15..29. Timeslot 0 on the E1 line carries framing data.

The following illustration shows how voice channel data is assigned to timeslots:

## T1/E1 signaling information routing (PRI mode)

If NetworkInterface.T1E1[x].SignalingType = PRI, signaling information is routed differently to accommodate an ISDN common channel signaling configuration, where CCS
signaling packets are transmitted in the D channel.

In PRI mode, the trunk signaling streams are not used. In this case, each trunk signaling stream has zero timeslots.

On CG 6060C boards, framer signaling is hard wired to internal HDLCs when the board runs in PRI mode. Refer to the PRI mode switch model. HDLC signaling is automatically terminated by an internal HDLC.

## Default connections (PRI mode)

If a board is configured for standalone operation (Clocking.HBus.ClockMode = STANDALONE), the DSPs and trunks are connected as shown in the following table.

Note: The SwitchConnections keyword can override this setting.

The exact settings for CG 6060C boards configured as T1 or E1 depend upon the NetworkInterface.T1E1[x].SignalingType keyword setting.

The following table shows the default routing for CG 6060C boards in PRI mode:

Trunk type | Full duplex connection between trunk voice information and the DSP resources...
--- | ---
T1 | Trunk 1: 0:0..22 => 65:0..22, Trunk 2: 4:0..22 => 65:24..46, Trunk 3: 8:0..22 => 65:48..70, Trunk 4: 12:0..22 => 65:72..94, Trunk 5: 16:0..22 => 65:96..118, Trunk 6: 20:0..22 => 65:120..142, Trunk 7: 24:0..22 => 65:144..166, Trunk 8: 28:0..22 => 65:168..190, Trunk 9: 32:0..22 => 65:192..214, Trunk 10: 36:0..22 => 65:216..238, Trunk 11: 40:0..22 => 65:240..262, Trunk 12: 44:0..22 => 65:264..286, Trunk 13: 48:0..22 => 65:288..310, Trunk 14: 52:0..22 => 65:312..334, Trunk 15: 56:0..22 => 65:336..358, Trunk 16: 60:0..22 => 65:360..382, | 64:0..22 => 1:0..22 64:24..46 => 5:0..22 64:48..70 => 9:0..22 64:72..94 => 13:0..22 64:96..118 => 17:0..22 64:120..142 => 21:0..22 64:144..166 => 25:0..22 64:168..190 => 29:0..22 64:192..214 => 33:0..22 64:216..238 => 37:0..22 64:240..262 => 41:0..22 64:264..286 => 45:0..22 64:288..310 => 49:0..22 64:312..334 => 53:0..22 64:336..358 => 57:0..22 64:360..382 => 61:0..22
E1 | Trunk 1: 0:0..29 => 65:0..29, Trunk 2: 4:0..29 => 65:30..59, Trunk 3: 8:0..29 => 65:60..89, Trunk 4: 12:0..29 => 65:90..119, Trunk 5: 16:0..29 => 65:120..149, Trunk 6: 20:0..29 => 65:150..179, Trunk 7: 24:0..29 => 65:180..209, Trunk 8: 28:0..29 => 65:210..239, Trunk 9: 32:0..29 => 65:240..269, Trunk 10: 36:0..29 => 65:270..299, Trunk 11: 40:0..29 => 65:300..329, Trunk 12: 44:0..29 => 65:330..359, Trunk 13: 48:0..29 => 65:360..389, Trunk 14: 52:0..29 => 65:390..419, Trunk 15: 56:0..29 => 65:420..449, Trunk 16: 60:0..29 => 65:450..479 | 64:0..29 => 1:0..29 64:30..59 => 5:0..29 64:60..89 => 9:0..29 64:90..119 => 13:0..29 64:120..149 => 17:0..29 64:150..179 => 21:0..29 64:180..209 => 25:0..29 64:210..239 => 29:0..29 64:240..269 => 33:0..29 64:270..299 => 37:0..29 64:300..329 => 41:0..29 64:330..359 => 45:0..29 64:360..389 => 49:0..29 64:390..419 => 53:0..29 64:420..449 => 57:0..29 64:450..479 => 61:0..29

On CG 6060C boards, the framer signaling is hard wired to internal HDLCs when the board runs in PRI mode.

Note: The CG 6060C board does not allow signaling streams to be connected to the CT bus.