# Switching errors (0x0C00)

The following table lists the switching errors (0x0C00):

Error name | Hex | Description | Category
--- | --- | --- | ---
SWITCH_MGR_ERROR_INVALID_PARAM | 0x0C01 | Invalid switching command. | 1
SWITCH_MGR_ERROR_OUT_OF_MEMORY | 0x0C02 | No more memory. | 3
SW_ERR_OUT_OF_MEMORY | 0x0C20 | Switching ran out of memory. | 3
SW_ERR_HARDWARE_NOT_FOUND | 0x0C21 | Switching hardware not found. | 3
SW_ERR_TIMESLOT_IN_USE | 0x0C22 | Internal switching error. | 3
SW_ERR_UNREACHABLE_TERMINAL | 0x0C23 | Internal switching error. | 3
SW_ERR_WIRE_NOT_INTERCHANGER | 0x0C24 | Internal switching error. | 3
SW_ERR_INVALID_TERMINALID | 0x0C25 | Internal switching error. | 3
SW_ERR_INVALID_OPERATION | 0x0C26 | Internal switching error. | 3
SW_ERR_NOT_POSSIBLE | 0x0C27 | TDM path not found. | 1
SW_ERR_OUT_OF_BOUNDS | 0x0C28 | Internal switching error. | 3
SW_ERR_STORE_EXCEEDED | 0x0C29 | Internal switching error. | 3
SW_ERR_WRONG_RECORD_TYPE | 0x0C2A | Internal switching state error. | 3
SW_ERR_NO_PATH | 0x0C2B | TDM path not found. | 1
SW_ERR_NO_SUCH_HOP | 0x0C2C | Internal switching state error. | 3
SW_RECORD_NOT_FOUND | 0x0C2D | Internal switching state error. | 3
SW_ERR_INVALID_OBJECT_STATE | 0x0C2E | Internal switching state error. | 3
SW_ERR_INVALID_PARAMETER | 0x0C2F | Internal switching state error. | 3
SW_ERR_MAPPING_FAILED | 0x0C30 | Internal switching error. | 3
SW_ERR_VIRTUAL_NOT_MAPPED | 0x0C31 | Internal switching error. | 3
SWITCH_MGR_ERR_NOT_ENABLED | 0x0C32 | Hardware or EEPROM fault during initialization. | 3
SW_ERR_TIMESLOTS NOT_AVAILABLE | 0x0C33 | Internal switching state error. | 3
SW_ERR_INVALID_STREAM | 0x0C34 | Stream does not exist. | 1
SW_ERR_PHYSICAL_TO_LOGICAL_MAP_FAILED | 0x0C35 | Internal switching error. | 3
SW_ERR_DEVICE_ERROR | 0x0C36 | Internal signaling DSP error. | 3
SW_ERR_NOT_SUPPORTED | 0x0C37 | Internal switching error. | 3
SW_ERR_NO_SUCH_TIMESLOT | 0x0C38 | Internal switching error. | 3
SWI_FAILED_TO_INITIALIZE | 0x5000 | Switching system initialization error. | 3