# slotStatus

Hot Swap status from the Hot Swap state machine.

#### Syntax

Integer

#### Access

Read-only

#### OID

p.3.1.1.4.n.m, where n is the index of this segment in the Bus Segment table and m is the index of the slot in this segment.

#### Details

Valid values:

Value | Status
--- | ---
1 | Online.
2 | Online Pending. The board coming online is in progress.
3 | Failed.
4 | Offline. The board is turned off and can be extracted.
5 | Offline Pending. Waiting for activity to stop (can be time consuming).
6 | Extracted.