# IP manager errors (0x1200)

The following table lists the IP manager errors (0x1200):

Error name | Hex | Description | Category
--- | --- | --- | ---
IPMGR_ERROR_OUT_OF_MEMORY | 0x1200 | Memory allocation error. | 3
IPMGR_ERROR_INVHANDLE | 0x1201 | Invalid resource handle. | 3
IPMGR_ERROR_INVSTATE | 0x1202 | Invalid state for operation. | 3
IPMGR_ERROR_INVKEY | 0x1203 | Lower interface key invalid. | 3
IPMGR_ERROR_LEV1DEFINE | 0x1204 | Level 1 driver define error. | 3
IPMGR_ERROR_TXOVERFLOW | 0x1205 | Transmit overflow. | 3
IPMGR_ERROR_DUPLICATE | 0x1206 | Duplicate resource type registered. | 4
IPMGR_ERROR_NOSUCHTYPE | 0x1207 | Invalid resource type. | 3
IPMGR_ERROR_NOROUTE | 0x1208 | No route available. | 4
IPMGR_ERROR_DUPNAME | 0x1209 | Duplicate resource or CPT name. | 3
IPMGR_ERROR_DUPHASHKEY | 0x120A | Duplicate hash key. | 3
IPMGR_ERROR_ARPERROR | 0x120B | ARP lookup problem. | 3
IPMGR_ERROR_INVNAME | 0x120C | Invalid resource name. | 3
IPMGR_ERROR_INVLENGTH | 0x120D | Packet size is less than or equal to 0, or greater than or equal to 1518. | 1
IPMGR_ERROR_LINKDOWN | 0x120E | Ethernet link is down. | 5
IPMGR_ERROR_SENDTOMBX | 0x120F | Failed to send to another task's mailbox. | 4
IPMGR_ERROR_RXTXD_BUF_LIMIT | 0x1210 | Failed to add to RXTXD buffer chain. | 3
IPMGR_ERROR_INVRXTXD | 0x1211 | Invalid RXTXD pointer passed. | 3
IPMGR_ERROR_RXTXD_ADJUST | 0x1212 | Error in trying to adjust the RXTXD buffer pointer. | 3
IPMGR_ERROR_INVMSGTYPE | 0x1213 | IP manager received an unknown message type. | 3
IPMGR_IPROUTE_ADDFAIL | 0x1214 | Unable to add the IP route to the table. | 4
IPMGR_ERROR_IPCHKSUM | 0x1215 | IP header checksum error. | 1
IPMGR_ERROR_TTLEXPIRE | 0x1216 | IP TTL expired. | 1
IPMGR_ERROR_CU_TIMEOUT | 0x1218 | 82559 Ethernet command timeout. | 3
IPMGR_INVALID_FUNCTION | 0x1219 | Unsupported function. | 1
IPMGR_ERROR_MAX_CONPTS | 0x121A | Maximum number of Ethernet connections has been exceeded. | 1
IPMGR_ETH1_LINK_FAIL | 0x121B | Status message – Ethernet link 1 is down. | 5
IPMGR_ETH2_LINK_FAIL | 0x121C | Status message – Ethernet link 2 is down. | 5
IPMGR_ETH1_LINK_ACTIVE | 0x121D | Status message – Ethernet link 1 is up. | -
IPMGR_ETH2_LINK_ACTIVE | 0x121E | Status message – Ethernet link 2 is up. | -
IPMGR_ERROR_MBOX_PKT_DROP | 0x1220 | Mailbox overflow. IP packet dropped. | 4
IPMGR_ERROR_NOTFOUND | 0x1221 | Entry not found. | 3
IPMGR_ERROR_INVPARAM | 0x1222 | ICMP v6 parameter error. | 3
IPMGR_ERROR_CHECKSUM_FAIL | 0x1223 | Bad checksum on received IPv6 ICMP packet. | -
IPMGR_IPV4ARP_INVENTRY | 0x1224 | Invalid ARP table entry. | 3
IPMGR_IPV4ARP_INVEVENT | 0x1225 | ARP state machine received invalid event. | 3
IPMGR_ERROR_INVCOMMAND | 0x1226 | IP Manager received unknown command. | 3
IPMGR_ERROR_ETHDRIVER | 0x1227 | Ethernet driver error. | 3
IPMGR_ERROR_OUT_OF_BUFFERS | 0x1228 | Ethernet static buffer pool exhausted. | 3
IPMGR_ERROR_BUFFERPOOL_ERROR | 0x1229 | Ethernet static buffer pool internal error. | 3
IPMGR_ERROR_NDERROR | 0x1280 | IPv6; Neighbor discovery error. | 3
IPMGR_ERROR_INVNEXTHDR | 0x1281 | IPv6; Invalid next header type. | 3
IPMGR_PROTOCOL_VIOLATION | 0x1282 | IPv6; Protocol error. | 3
IPMGR_IPV6DEST_NOTFOUND | 0x1283 | IPv6; Destination entry for IP address not found. | 3
IPMGR_ERROR_INV_IPV6ADDR | 0x1284 | IPv6; Invalid address. | 3
IPMGR_IPV6ND_NOTFOUND | 0x1285 | IPv6; Neighbor discovery (ND) entry for IP address not found. | 3
IPMGR_IPV6ND_INVEVENT | 0x1286 | IPv6; Invalid neighbor discovery (ND) event. | 3
IPMGR_IPV6IF_NOTFOUND | 0x1288 | IPv6; Interface entry not found in the Interface table. | 3
IPMGR_IPV6MC_NOTFOUND | 0x1289 | IPv6; Multicast address not found in the Interface table. | 3
IPMGR_IPV6ND_DUPADDRDET | 0x128A | IPv6; Duplicate address detected. | 3
IPMGR_IPV6ND_TIMERERR | 0x128B | IPv6; Error with neighbor discovery (ND) timer. | 3
IPMGR_IPV6RTR_TIMERERR | 0x128C | IPv6; Error with router timer. | 3
IPMGR_SEC_POL_DISCARD | 0x12A0 | IPSec; Transmit packet dropped; policy states that the packet is to be discarded. | 3
IPMGR_SEC_SA_NOT_FOUND | 0x12A1 | IPSec; No security association (SA) can be found. | 3
IPMGR_SEC_PROTO_UNKNOWN | 0x12A2 | IPSec; Unsupported security protocol. | 3
IPMGR_SEC_INVALID_SPI | 0x12A4 | IPSec; Receive packet with unknown SPI value. | 3
IPMGR_SEC_AUTH_FAILED | 0x12A5 | IPSec; Authentication failed. | 3
IPMGR_SEC_INVALID_PARAM | 0x12A6 | IPSec; Invalid parameter. | 3
IPMGR_SEC_POLICY_VIOLATION | 0x12A7 | IPSec; Policy disallows packet. | 3
IPMGR_SEC_SA_INVALID_STATE | 0x12A9 | IPSec; Security association (SA) not active. | 3
IPMGR_SEC_INTERNAL_ERROR | 0x12AA | IPSec; Inconsistency. | 3
IPMGR_SEC_BAD_BLOCK_ALIGNMENT | 0x12AB | IPSec; Block size violation. | 3
IPMGR_SEC_DECRYPT_FAILED | 0x12AC | IPSec; Invalid ESP plain text. | 3