# Framer manager errors (0x0D00)

The following table lists the framer manager errors (0x0D00):

Error name | Hex | Description | Category
--- | --- | --- | ---
FRAMER_MGR_ERROR_INVALID_PARAM | 0x0D01 | Invalid framer command. | 3
FRAMER_MGR_ERROR_OUT_OF_MEMORY | 0x0D02 | No more memory. | 3
FRMR_MGR_ERR_INVALID_PARAMETER | 0x0D03 | Parameters passed to the function do not match the requirements. | 3
FRMR_MGR_ERR_ILLEGAL_FRAMER_INDEX | 0x0D04 | Framer INDEX outside the range of valid framers. | 3
FRMR_MGR_ERR_PREV_FRAMER_DEFINED | 0x0D05 | A framer instance already exists at this index. | 3
FRMR_MGR_ERR_UNRECOG_FRAMER_TYPE | 0x0D06 | Attempted to create an invalid framer type. Framer type must be T1 or E1. | 3
FRMR_MGR_ERR_NO_CONFIG_BUF | 0x0D07 | No configuration buffer to send to init code. | 3
FRMR_MGR_ERR_NONE_ALLOCATE | 0x0D08 | Call to a command with a framer instance that does not exist. | 3
FRMR_MGR_ERR_UNABLE_TO_START_1SEC_THREAD | 0x0D09 | Unable to start the thread for a 1 second process. | 3
FRMR_MGR_ERR_UNABLE_TO_START_IRQ_THREAD | 0x0D0A | Unable to start the thread for a 1 second process. | 3
FRMR_MGR_ERR_UNABLE_TO_CREATE_1SEC_LIST | 0x0D0B | Unable to create a new function list for a 1 second process. | 3
FRMR_MGR_ERR_UNABLE_TO_CREATE_IRQ_LIST | 0x0D0C | Unable to create a new function list for an IRQ process. | 3
FRMR_MGR_ERR_UNABLE_TO_CREATE_EVENT_HDL | 0x0D0D | Unable to create an event handle for an IRQ DPC code. | 3
FRMR_MGR_ERR_UNABLE_TO_CREATE_DPC_LIST | 0x0D0E | Unable to create a list to handle DPCs. | 3
FRMR_MGR_ERR_NO_BUF | 0x0D0F | Command expected a buffer that was not present. | 3
FRMR_MGR_ERR_UNABLE_TO_ENABLE_IRQ | 0x0D10 | Could not hook into an IRQ chain. | 3