# saiAsrGetRecognitionStartTimer

Retrieves whether the recognizer starts its no-input timer at the beginning of the recognizer session or waits for a call to saiStartTimerRecognizer. For more information, refer to Implementing a barge-in enabled prompt.

#### Prototype

DWORD saiAsrGetRecognitionStartTimer ( SAI_RECOGNIZER_HANDLE recog H d, BOOL *value )

Argument | Description
recogHd | Handle associated with a recognizer resource.
value | Pointer to one of the following values: TRUE: Recognizer starts its no-input timer when the application calls saiStartRecognizer. FALSE: Recognizer starts its no-input timer when the application calls saiStartTimerRecognizer.

#### Return values

Return value | Description
SUCCESS |
SAIERR_INVALID_PARAMETER | One of the specified arguments is invalid.
SAIERR_UNSUPPORTED_SPEECH_PARAMETER | Recognizer engine does not support the specified parameter.

#### See also

saiAsrSetRecognitionStartTimer