# ACU_DIGIT_IN

This topic describes:

- ACU_DIGIT_IN protocol variants

- ACU_DIGIT_IN macro descriptions and Q.931 IE

#### Purpose

Receives called number digits in overlap receiving mode.

#### Conn_id

An allocated call.

## ACU_DIGIT_IN protocol variants

The following table lists the variants under which each macro is supported for this primitive. In this table, NT = NT side only, TE = TE side only, and x = both NT and TE sides.

Macro | 4 E S S | E 1 0 | N I 2 | D M S | E T S I | V N 6 | H K G | A U S T E L 1 | N T T | K O R E A | T A I W A N | Q S I G | D P N S S | T 1 6 0 7
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Acu_digit_in_a_digit, Acu_digit_in_digit_size |  |  |  |  | x | x | TE |  | NT | x | x | x | x |
Acu_digit_in_a_display, Acu_digit_in_display_size |  |  |  |  | x | x | TE |  | NT | x | x | x |  |
Acu_digit_in_a_display_list |  |  |  |  | x | x |  |  | NT | x | x | x |  |
Acu_digit_in_a_q931, Acu_digit_in_q931_size |  |  |  |  | x | x | TE |  | NT | x | x | x | x |
Acu_digit_in_digit_type |  |  |  |  | x | x |  |  |  | x | x | x |  |
Acu_digit_in_digit_plan |  |  |  |  | x | x |  |  |  | x | x | x |  |
Acu_digit_in_sending_complete |  |  |  |  | x | x | TE |  | NT | x | x | x | x |
Acu_digit_in_x_display_nb |  |  |  |  | x | x | TE |  | NT | x | x | x |  |
Acu_digit_in_x_display_size[i] |  |  |  |  | x | x | TE |  | NT | x | x | x |  |
Acu_digit_in_x_display_total_size |  |  |  |  | x | x | TE |  | NT | x | x | x |  |
Acu_digit_in_x_display_type[i] |  |  |  |  | x | x | TE |  | NT | x | x | x |  |
Acu_digit_in_x_p_display[i] |  |  |  |  | x | x | TE |  | NT | x | x | x |  |

## ACU_DIGIT_IN macro descriptions and Q.931 IE

Macro | Description | Q.931 IE
--- | --- | ---
Acu_digit_in_a_digit, Acu_digit_in_digit_size | Address and size of digit string. | Called party number
Acu_digit_in_a_display, Acu_digit_in_display_size | Pointer to (and size of) buffer containing ISDN display information (optional). | Display
Acu_digit_in_a_display_list | Pointer to display structure. | Display
Acu_digit_in_a_q931, Acu_digit_in_q931_size | Pointer to (and size of) buffer containing raw data of incoming Q.931 message. | Does not map to an IE.
Acu_digit_in_digit_type | Called number type. | Called party number
Acu_digit_in_digit_plan | Called number plan. | Called party number
Acu_digit_in_sending_complete | Indicates if the sending-complete information element was received (ON/OFF). | Sending complete
Acu_digit_in_x_display_nb | Number of present occurrences. | Display
Acu_digit_in_x_display_size[i] | Size of occurrence i (optional). | Display
Acu_digit_in_x_display_total_size | Total size of the stored strings. | Display
Acu_digit_in_x_display_type[i] | Type of display i. | Display
Acu_digit_in_x_p_display[i] | Pointer to occurrence i. | Display