# dsx1SendCode

Type of code sent across the DS1 interface by the device.

#### Syntax

Integer

#### Access

Read/write

#### OID

p.6.1.7.n, where n = the index number of the DS1 interface.

#### Details

Valid values include:

Type | Value | Description
--- | --- | ---
dsx1SendNoCode | 1 | Sending looped or normal data.
dsx1SendLineCode | 2 | Sending a request for a line loopback.
dsx1SendPayloadCode | 3 | Sending a request for a payload loopback.
dsx1SendResetCode | 4 | Sending a loopback termination request.
dsx1SendQRS | 5 | Sending a quasi-random signal (QRS) test pattern.
dsx1Send511Pattern | 6 | Sending a 511 bit fixed test pattern.
dsx1Send3in24Pattern | 7 | Sending a fixed test pattern of 3 bits set in pattern of 24.
dsx1SendOtherTestPattern | 8 | Sending a test pattern other than those described by this object.

Note: The SNMP agent returns dsx1SendNoCode (normal data). Loopback is not supported.