# dsx1LineStatus

Status of the interface.

#### Syntax

Integer (1..8191)

#### Access

Read-only

#### OID

p.6.1.10.n, where n = the index number of the DS1 interface.

#### Details

This value provides loopback, failure, received alarm, and transmitted alarm information. Possible status values include:

Status | Value | Description
--- | --- | ---
dsx1NoAlarm | 1 | No alarm present.
dsx1RcvFarEndLOF | 2 | Yellow alarm. Not supported.
dsx1XmtFarEndLOF | 4 | Near end sending LOF indication. Not supported.
dsx1RcvAIS | 8 | Far end sending AIS (blue). Not supported.
dsx1XmtAIS | 16 | Near end sending AIS.
dsx1LossOfFrame | 32 | Near end LOF (red alarm).
dsx1LossOfSignal | 64 | Near end loss of signal.
dsx1LoopbackState | 128 | Near end is looped.
dsx1T16AIS | 256 | E1 TS16 AIS.
dsx1RcvFarEndLOMF | 512 | Far end sending TS16 LOMF. Not supported.
dsx1XmtFarEndLOMF | 1024 | Near end sending TS16 LOMF. Not supported.
dsx1RcvTestCode | 2048 | Near end detects a test code.
dsx1OtherFailure | 4096 | Interface status not defined.

Note: Far end is not supported.