# Error type FF00 (Solaris only)

The following table lists FF00 type (host driver) errors:

Error code | Error name | Additional information returned | Category
--- | --- | --- | ---
-22 | AGERR_MSG_BALANCE_LOST | Channel, message. | 3
-42 | AGERR_LESS_THAN_48_BYTES | SRAM words left. | 3
-43 | AGERR_RECEIVE_MSG_COUNT | Count left, next message, SRAM location. | 3
-44 | AGERR_AGMSG_DATA | Buffer count, parameter count. | 3
-81 | AGERR_WRITE_QUEUE_EMPTY | AGHW is currently doing a write, but write queue is empty. | 3
-100 | AGERR_NO_STREAMS_MSG_BLOCK | Channel, message. | 3
-101 | AGERR_FLOW_CONTROLLED | Channel, message. | 3
-102 | AGERR_CANT_RESPOND_TO_MCTL | Command, AGERR_x. | 3
-421 | AGXERR_IDLE_CHANNEL | Channel, message. | 3
-422 | AGXERR_BAD_MSG_PARM | Pointer to open context, channel | 3
-441 | AGXERR_BAD_CHANNEL_NUMBER | Channel, message. | 3
-481 | AGXERR_CHANNEL_INFO | Pointer to open context, channel. | 3
-482 | AGXERR_ORPHAN_CHNL_CREATED | Board number, channel. | 3
-483 | AGXERR_BAD_MSG_SIZE | Size. | 3
-484 | AGXERR_BAD_MSG | Channel, message. | 3
-485 | AGXERR_BAD_MSG_UNIT | Unit. | 3
-486 | AGXERR_INVALID_STREAMS_MSG | STREAMS message type. | 3
-501 | AGXERR_FLOW_CONTROLLED | Channel, message. | 3
-603 | AGSERR_INVALID_MSGPARMS | Parameter count. | 3
-610 | AGSERR_PREVCLOSEFAILED | Not used. | 3
-612 | AGSERR_ORPHAN_CHNL_CREATED | Channel. | 3
-613 | AGSERR_SERVICE_PRIMITIVE | Primitive. | 3
-614 | AGSERR_WRONG_CHANNEL | Channel. | 3
-620 | AGSERR_BAD_MSG_UNIT | Unit. | 3
-621 | AGSERR_UNEXPECTED_SVC_PRIM | Primitive. | 3
-622 | AGSERR_DESTROY_CHNL_FAILED | Channel. | 3
-623 | AGSERR_UNEXPECTED_EVENT | Event. | 3
-630 | AGSERR_UNKNOWN_ERROR | Error. | 3