# NTT (Japan) caller ID data

The following table describes the caller ID format for NTT (Japan):

Parameter | Values | Type | Length | Field
Calling line number | Calling number identity | 0x02 | up to 30 | Receive: NCC_CALL_STATUS.callingaddr
Reason for absence of number | O - Unavailable P - Private C - Coin/card public telephone origin S - Service status | 0x04 | 1 | Receive: NCC_CALL_STATUS.ANIpresentation
Calling name | Calling name | 0x07 | up to 30 | Receive: NCC_CALL_STATUS.callingname
Reason for absence of name | O - Unavailable P - Private C - Coin/card public telephone origin S - Service status | 0x08 | 1 | Receive: NCC_CAS_EXT_CALL_STATUS.NAMEpresentation
Called number (DDN) | The number of called party, including DDI number | 0x09 | up to 30 | Receive: NCC_CALL_STATUS.calledaddr
Date/time | MMDDhhmm | 0x01 | 8 | Receive: NCC_CAS_EXT_CALL_STATUS.datetime
Redirecting number | The last redirecting party | 0x0B | up to 30 | Receive: NCC_CAS_EXT_CALL_STATUS.redirectingaddr
Reason for redirection | 0x00 - Undefined 0x01 - Busy 0x02 - Unanswered 0x15 - Unconditional | 0x0B | 1 | Receive: NCC_CAS_EXT_CALL_STATUS.redirectingreason
Calling number extended | Calling user type. 0xTP where: T = Type of number. Values: 0 - Unknown 1 - International 2 - Domestic 3 - Network 4 - Local 6 - Abbreviated P = Numbering plan. Values: 0 - Unknown 1 - ISDN 3 - Data 4 - Telex 8 - Domestic 9 - Private | 0x21 | 1 | Receive: NCC_CAS_EXT_CALL_STATUS.usercategory
Public message |  | 0x24 | up to 30 | Receive: NCC_CAS_EXT_CALL_STATUS.carrierID