# imgtStop

Stops a management session initiated with imgtStart.

#### Prototype

DWORD imgtStop ( CTAHD ctahd )

Argument | Description
ctahd | Context handle returned by ctaCreateContext.

#### Return values

Return value | Description
SUCCESS |
CTAERR_INVALID_HANDLE | The specified context handle is invalid.

#### Events

Event | Description
IMGTEVN_RCV_MESSAGE | An IMGT message with the code IMGT_STOPPED is returned in response to imgtStop. The message status field contains SUCCESS. This message indicates that the management session has been stopped.

#### Example

void ResetimgtConfiguration( CTAHD ctahd )
{
DWORD ret;
char *errortext="";
/* stop receiving any events on the appropriate context */
ret = imgtStop( ctahd );
if (ret != SUCCESS)
{
ctaGetText( ctahd, ret, (char *) errortext, 40);
printf( "imgtStop failure: %s\n",errortext );
exit( 1 );
}
/* wait for IMGTEVN_RCV_MESSAGE */
...
}

#### See Also

imgtStart