# dsx1CurrentPCVs

Number of path coding violations.

#### Syntax

Gauge

#### Access

Read-only

#### OID

p.7.1.7.n, where n = the index number of the DS1 interface.

#### Details

A path coding violation error event is a frame synchronization bit error in the D4 and E1-noCRC formats or a CRC or frame synch.bit error in the ESF and E1-CRC formats. Also known as CV-P (see ANSI T1.231, Section 6.5.2.1).