# adiStartTones

Starts generating one or more tones.

#### Supported board types

- AG

- CG

#### Prototype

DWORD adiStartTones ( CTAHD ctahd, unsigned count, ADI_TONE_PARMS *parms)

Argument | Description
ctahd | Context handle returned by ctaCreateContext or ctaAttachContext.
count | Number of entries in the parms array.
parms | Pointer to an array of tones defined by the following structure (NULL designates default values): typedef struct { DWORD size ; /* size of this structure */ DWORD freq1; /* first frequency (Hz) */ INT32 ampl1; /* level of first tone (dBm) */ DWORD freq2; /* second frequency (Hz) */ INT32 ampl2; /* level of second tone (dBm) */ DWORD ontime; /* on duration of DTMF tone (ms) */ DWORD offtime; /* off duration of DTMF tone (ms) */ INT32 iterations;/* times to repeat above; -1 = forever*/ } ADI_TONE_PARMS; Refer to ADI_TONE_PARMS for field descriptions.

#### Return values

Return value | Description
SUCCESS |
ADIERR_INVALID_CALL_STATE | Function not available in the current call state.
CTAERR_FUNCTION_ACTIVE | Function already active.
CTAERR_INVALID_CTAHD | Context handle is invalid.
CTAERR_INVALID_STATE | Function not available in the current port state.
CTAERR_OUTPUT_ACTIVE | Function failed because there is another active output function.
CTAERR_SVR_COMM | Server communication error.

#### Events

Event | Description
ADIEVN_TONES_DONE | The value field contains any of the following reasons: CTAERR_xxx or ADIERR_xxx Tone generation failed. CTA_REASON_FINISHED Tones generated. CTA_REASON_STOPPED Tone generation stopped by adiStopTones.

#### Details

The following DSP
file must be loaded to the board before running adiStartTones:

For these boards... | Load this DSP file...
AG | tone.m54
CG | tone.f54

See DSP file summary for DSP file descriptions. Refer to the board installation and developer's manual for a table of MIPS
usage for all functions.

Use this function to start generating a sequence of tones, each consisting of one or two frequencies and an iteration count. The DONE event is generated when the tone sequence completes.

Each tone within the sequence comprises an ontime and an offtime, as well as an iterations count, all of which are contained in the ADI_TONE_PARMS structure. The final iteration is complete when the offtime expires. To generate a tone continuously, set iterations to -1 and specify an offtime of 0 (zero).

Use adiStopTones to prematurely terminate tone generation.

For more information, refer to Generating tones.

#### See also

adiStartDTMF

#### Example

/* generates an Intralata Reorder SIT per BellCore */
int myPlaySITReorder( CTAHD ctahd )
{
ADI_TONE_PARMS p[3] = {0};
CTA_EVENT event;
int tonecnt = 3;
p[0].freq1 = 914; p[0].ampl1 = -24; p[0].ontime = 275; p[0].iterations = 1;
p[1].freq1 = 1429; p[1].ampl1 = -24; p[1].ontime = 380; p[1].iterations = 1;
p[2].freq1 = 1777; p[2].ampl1 = -24; p[2].ontime = 380; p[2].iterations = 1;
if( adiStartTones( ctahd, tonecnt, p ) != SUCCESS )
return MYFAILURE;
while( 1 )
{
myGetEvent( &event ); /* see ctaWaitEvent example */
switch( event.id )
{
case ADIEVN_TONES_DONE:
if( event.value == CTA_REASON_RELEASED )
return MYDISCONNECT; /* call has been terminated */
else if( CTA_IS_ERROR( event.value ) )
return MYFAILURE; /* API error */
else
return SUCCESS; /* stopped normally */
break;
}
}
}