# ADI_DIAL_PARMS

#### Dependent function: adiStartDial

Field name | Type | Default | Units | Description
--- | --- | --- | --- | ---
breaktime | DWORD | 60 | ms | Break (on-hook) duration for dial pulses. Valid AG board and CG board range is 0 through 30000.
dialtonewait | DWORD | 5000 | ms | Maximum time to wait for dial tone (; character). Valid range is 0 through 65535.
dtmfampl1 | INT32 | -6 | dBm | Amplitude of the low frequency component of the DTMF pair. Valid AG board and CG board range is -54 through -3.
dtmfampl2 | INT32 | -4 | dBm | Amplitude of the high frequency component of the DTMF pair. Valid AG board and CG board range is -54 through -3.
dtmfofftime | DWORD | 80 | ms | Duration of the silence time between each digit. Valid AG board and CG board range is 0 through 65534.
dtmfontime | DWORD | 80 | ms | Duration of each DTMF or MF digit. Valid AG board and CG board range is 0 through 65534.
flashtime | DWORD | 500 | ms | Amount of time to assert the on-hook signaling pattern for a flash (! character). Valid AG board and CG board range is 0 through 65535.
interpulse | DWORD | 700 | ms | Inter-digit time for pulsed dialing. Valid AG board and CG board range is 0 through 30000.
longpause | DWORD | 5000 | ms | Amount of delay associated with the . (period) character. Valid range is 0 through 65535.
maketime | DWORD | 40 | ms | Make (off-hook) duration for dial pulses. Valid AG board and CG board range is 0 through 30000.
method | DWORD | 0 | mask | Type of signaling. 0=DTMF 1=Pulse 2=MF (US)
reserved | DWORD | 0 | internal | Do not modify.
shortpause | DWORD | 2000 | ms | Amount of delay associated with the , (comma) character. Valid range is 0 through 65535.
tonebandw1 | DWORD | 40 | Hz | Bandwidth of the first frequency of the dial tone detector. Valid AG board and CG board range is 20 through 800.
tonebandw2 | DWORD | 40 | Hz | Bandwidth of the second frequency of the dial tone detector. Valid AG board and CG board range is 20 through 800.
tonefreq1 | DWORD | 350 | Hz | First (or only) dial tone frequency. Valid AG board and CG board range is 330 through 3600.
tonefreq2 | DWORD | 440 | Hz | Second dial tone frequency. Set this value to 0 (zero) to detect a single frequency. Valid AG board and CG board range is 330 through 3600.
tonequalampl | INT32 | -28 | dBm | Minimum signal amplitude to qualify for dial tone detection. Valid AG board and CG board range is -40 through 0.
tonequaltime | DWORD | 50 | ms | Minimum duration of a qualified tone to be considered dial tone. Valid range is 0 through 32767.
tonereflevel | DWORD | 0xB000 | IDU | Do not modify.
tonetotaltime | DWORD | 0 | ms | Detects interrupted dial tones (stuttered dial tone) in certain countries. Defaults to 0 (zero), which indicates that dialing can proceed as soon as a dial tone is detected without waiting for stuttered dial tone to end. If set to a non-zero value, the value represents the total qualification time for dial tone, and the following occurs: Only precise dialtone detection is used. If dialtone disappears, requalify until dialtonewait expires. If dialtone lasts for totaltime, proceed with dialing.