# Installing Dell R410 Driver (Broadcom)

If you are using the Dell R410 server, follow the steps below to install the required driver.

1. Download the Dell410 driver (Broadcom) from support.dell.com. Burn them to a CD.

2. Copy the netxtreme2-5.0.17.tar.gz file to the hard drive and untar the driver.

3. Go to the bnx2-1.9.20B directory and in the src directory type make.

4. Type make install to install the driver.

5. Reboot the server.