# Configuring the PowerMedia WMS

Once the system is fully booted up, use another system that is accessible through the network to PowerMedia WMS to complete the basic configuration steps below.

1. Connect to the Web UI using the following URL:
   https://WMS_IP_Address

2. Connect to the Web UI. The login page appears.

3. Log in with admin for the username. Leave the password field blank. The Version Information page appears.

4. Select Network->Configure->Interfaces. The Interfaces page appears.

5. Click the button of the IP address associated with the Web UI (for example, 146.152.83.170). The Configure Network Interfaces page appears.

6. If your PowerMedia WMS was previously set up for DHCP, select Statically set IP address and provide the IP address and subnet mask. Select Enable RTP on IP Address. Click OK. A message similar to the following appears:
   The device configuration for eth0 has been updated.
   Note: if you change the IP address on which SIP or RTP is enabled, the host must be rebooted.

7. Select Network->Configure->Routes. The Routes page appears.

8. Click ADD ROUTE to create a new route. Enter the values associated with the route. Add as many routes as needed.

9. Click OK. A message is displayed indicating the route or routes that have been added.

10. When you are done adding routes, select System->Reboot Host. The Reboot Host page appears.

11. Select Clear HTTP Cache and click OK to reboot the system. It takes three to five minutes for the system to boot up and have the Web UI accessible again.

The PowerMedia WMS is ready to take calls at the IP address configured.