# Installing the Client Softphone

Follow the procedures below to install and configure a client softphone to call the PowerMedia WMS. These instructions use the Kapanga softphone as an example.

The PowerMedia WMS includes a trial version of the Kapanga softphone; the trial version lasts for 90 days (Windows® and Linux clients).

1. Locate the kapanga_client.zip at the following address:
   https://192.168.12.168/snowshore/apps/
   "192.168.12.168" is the IP address of the PowerMedia WMS.

2. Click the kapanga.zip file and choose to save or open the file.

3. If you saved the zip file, double-click the file to unzip it. If you selected open, the file automatically unzips.

4. Double-click the kapanga_client_setup.exe file. The Setup Wizard appears.

5. Follow the wizard to complete the installation. When complete, you can select to launch Kapanga Client Softphone.