AF. A predefined PPL software routine that performs a single, simple task, such as "Transmit Line Signaling" or "Allocate Digit Buffer." It is composed of standard software interrupts, calls, and data formats used by applications. Each AF has two values named "Arguments." AFs 1-50 are generic, and apply to all PPL components. AFs 51 and above apply to specific components. An AF is called "Atomic" because it is the smallest useful unit in PPL.