0x0061 Reject Reason

Used in:
PPL Event Indication message

Byte | Description
0, 1 | Tag 0x0060
2, 3 | Length 0x0002
4, 5 | Value[0, 1] Reject Reason 0x02 Admission Reject (ARJ) Indication 00 01 Called Party Not Registered 00 02 Invalid Permission 00 03 Request Denied 00 04 Undefined Reason 00 05 Caller Not Registered 00 06 Route Call To Gatekeeper 00 07 Invalid Endpoint Identifier 00 08 Resource Unavailable 00 09 Security Denial 00 0A QOS Control Not Supported 00 0B Incomplete Address 0x05 Bandwidth Reject (BRJ) Indication 00 01 Not Bound 00 02 Invalid Conference ID 00 03 Invalid Permission 00 04 Insufficient Resources 00 05 Invalid Revision 00 06 Undefined Reason

See Programmable Protocol Language.
An H.323 entity on the network that provides address translation and controls access to the network for H.323 terminals and other end points. The gatekeeper may also provide other services to the endpoints such as bandwidth management and locating gateways.
An H.323 terminal or gateway, or MCU. An endpoint can call and be called. It generates and/or terminates the information stream.