0x0272 Use SIP Registration Timeout

Use this TLV to specify the default registration expiration period in seconds that is used when no registration expiration period is specified. The default value is 0x00000E10 (3600 seconds).

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x0272
2, 3 | Length 0x0004
4-7 | Value[0-3] Registration Expiration Period (4 Bytes)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).