0x05F3 Vocabulary Index Read Information

This TLV is sent in the response to the Generic Card Query message. It indicates the number of files in the Vocabulary Index File (VIF) and checks the integrity of the VIF through a checksum.

Byte | Description
0, 1 | Tag: 0x05F3 - Vocabulary Index Read Information
2, 3 | Length: 0x0008
4-7 | Value[0-3] - Number of files in the Index file
8-11 | Value[4-7] - Vocabulary Index File checksum

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.