You are here: CSP Developer’s Guide: Internet Protocol > 5 Session-Initiation Protocol (SIP) Software > Reporting/Generating SIP Headers or Parameters

Reporting/Generating SIP Headers or Parameters

The section describes the following features that report or generate SIP headers or parameters.

• Host Notification of Selective SIP Header Information

• Via Heading Reporting

• Call-ID Reporting for Outbound SIP Calls

• Subject Header Field Access

• SIP Display Name Parameter in From Header

• Access To Contact Header

• SIP Access To Parameters in To Header

• Report and Control of P-Asserted and P-Access Network Info Headers

• SIP Remote Party ID and RPID Privacy for Outbound Calls

• Remote Party ID

Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.